# earth_rover

![earth_rover](https://pbs.twimg.com/media/Eqh29nYUUAA-9NE?format=jpg)

Mechanical warm, or just cubic macro pad.

* Keyboard Maintainer: [k.bigwheel](https://github.com/bigwheel)
* Build Guide: [bigwheel/earth\_rover](https://github.com/bigwheel/earth_rover)
* Hardware Supported: [無限の可能性 \| MxLEDBitPCB](https://swanmatch.github.io/MxLEDBitPCB/), Pro Micro
* Hardware Availability: [魔界鍵盤製作所 \- BOOTH](https://swanmatch.booth.pm/), [Pro Micro （コンスルー付き） \| 遊舎工房](https://yushakobo.jp/shop/promicro-spring-pinheader/)

Make example for this keyboard (after setting up your build environment):

    make earth_rover:default

Reset Pro Micro by reset button on ProMicroSocket (Red LED must light).

Flashing example for this keyboard:

    make earth_rover:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
