# Aya

![Aya](https://raw.githubusercontent.com/DanNixon/aya/main/docs/both_sides.jpg)

A column staggered, symmetrical split keyboard.

* Keyboard Maintainer: [Dan Nixon](https://github.com/dannixon)
* Hardware Supported: Aya PCB, Pro Micro
* Hardware Availability: CAD files [here](https://github.com/DanNixon/aya)

Make example for this keyboard (after setting up your build environment):

    make aya:default

Enter the bootloader in 2 ways:

* **Command**: Hold down both shift keys and press B
* **Physical reset button**: Briefly short the pads on the read of the PCB (directly behind the Pro Micro)

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
