# Jones v.0.3.1

![Jones, ANSI style](https://github.com/jpskenn/Jones/raw/master/assets/IMG_2204.jpeg)

![Jones, JP style](https://github.com/jpskenn/Jones/raw/master/assets/DSC_7189.jpeg)

A 60% keyboard combined with Ortho-Linear and Row-staggered. It has gapless R2-R3 row.  
GH60 case compatible PCB and keyplate.

* Keyboard Maintainer: [jpskenn](https://github.com/jpskenn)
* Hardware Supported: Jones PCB, Keyplate
* Hardware Availability: [GitHub](https://github.com/jpskenn/Jones), [BOOTH](https://jpskenn.booth.pm)

Make example for this keyboard (after setting up your build environment):

    make jones/v03_1:default
    
Flashing example for this keyboard ([using the command line](https://docs.qmk.fm/#/newbs_flashing?id=flash-your-keyboard-from-the-command-line)):

    make jones/v03_1:default:flash

To reset the keyboard into bootloader mode, press the reset switch on the underside.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
