# CU65

The CU65 is a customisable 65% that supports hotswap ISO and ANSI layouts on the same PCB.

* Keyboard maintainer: [rys](https://github.com/rys)
* Hardware supported: CU65 r2
* Hardware availability: [CapsUnlocked](https://caps-unlocked.com/cu65-r2/)

Make example for this keyboard (after setting up your build environment):

    make capsunlocked/cu65:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
