# Ergo42

![Ergo42](https://raw.githubusercontent.com/Biacco42/Ergo42/readme/readme_image/ergo42_image.jpg)

__The Answer to the Ultimate Question of Life, the Universe, and at least Keyboards.__  
A split 7x4 ortholinear keyboard. [Hardware project repo](https://github.com/Biacco42/Ergo42)

* Keyboard Maintainer: [Biacco42](https://github.com/Biacco42) [@Biacco42](https://twitter.com/Biacco42)
* Hardware Supported: Ergo42 PCB, Pro Micro ATmega32u4
* Hardware Availability: [Ergo42 PCB and case](https://github.com/Biacco42/Ergo42)

Make example for this keyboard (after setting up your build environment):

    make biacco42/ergo42/rev1:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
