# Keymap for Jones with VIA support

VIA supported basic keymap with external EEPROM.

## Layout

Japanese style "Wide" layout.

## Layers

- Base #1
- Base #2
- Base #3
- Lower
- Raise
- Adjust

## External EEPROM

I2C connected external EEPROM.

## LED lighting

4 LEDsfor layer indicator.  
2 for Left side and 2 for Right side.

## Rotary encoder

Supports up to 2 rotary encoders.  
Left bottom and Right bottom.

## Audio

Supports monophonic audio.  
"Music Mode" and "Audio Click" are enabled.
