# Nozbe Macropad handwired

![Nozbe Macropad](https://i.imgur.com/fUMtWmah.png)

4 key macropad with optional rotary encoder.

* Keyboard Maintainer: [rozPierog](https://github.com/rozPierog)
* Hardware Supported: Custom handwired 4 key (or 3 key + rotary encoder) pad
* Hardware Availability: *n/a*
* Github Repository: [NozbePad](https://github.com/rozPierog/NozbePad)

Make example for this keyboard (after setting up your build environment):

    make handwired/nozbe_macro:default

Flashing example for this keyboard:

    make handwired/nozbe_macro:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader in 1 way:

* **Short pins**: short RST and GND pins at the back
