# Axon

![Axon](https://i.imgur.com/VRVv9i9h.jpeg)

Axon v1.0 built with Durock T1 and GMK Bento

Axon is a compact 40% which uses through-hole components. Hardware repo can be found at https://github.com/thatfellarobin/axon.

* Keyboard Maintainer: [Robin Liu](https://github.com/thatfellarobin)

Make example for this keyboard (after setting up your build environment):

    make handwired/axon:default

## To reset into bootloader mode:

1. While plugged in, press and hold `BOOT` switch
2. While holding `BOOT`, press `RESET` and hold it for a second or two
3. Release `RESET`
4. Release `BOOT`
5. The keyboard should now be recognized as a USBasp programmer device.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
