# SNOP60

![SNOP60](https://i.imgur.com/2aBmgMah.png)

60% Universal PCB featuring Tsangan bottom row, 2x3u bar support, backlighting, RGB underglow, rotary encoder support, and two flex cutouts.

- Keyboard Maintainer: [Nasp](https://github.com/npspears)
- Hardware Supported: SNOP60 PCB
- Hardware Availability: [Checker Boards](https://www.checkerboards.xyz/SNOP60_p_65.html)

Make example for this keyboard (after setting up your build environment):

    make checkerboards/snop60:default

Flashing example for this keyboard:

    make checkerboards/snop60:default:flash

Enter the bootloader by pressing the reset button below the USB and JST connector.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
