# CherryB Studio CB87RGB

![cb87rgb](https://i.imgur.com/wG1qS4I.jpg)

A RGB TKL PCB including hotswap and solderable variant for CherryB Studio NEO87 and many compatible TKLs

* Keyboard Maintainer: [lunaticwhat](https://github.com/lunaticwhat)
* Hardware Supported: cb87rgb, atmega32u4
* Hardware Availability: [CherryB Studio](https://discord.gg/3gsCa8K)

Make example for this keyboard (after setting up your build environment):

    make cherrybstudio/cb87rgb:default

Flashing example for this keyboard:

    make cherrybstudio/cb87rgb:default:flash

## Accessing Bootloader Mode

To access Bootloader Mode, do one of the following:

* Tap the Reset switch mounted on the top side of the PCB to the left of the spacebar
* Hold the top left key of the keyboard while connecting the USB cable

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
