# ogurec keymap for left-sided PM placement

Make example for this keyboard (after setting up your build environment):

    make ogurec/left_pm:default

Flashing example for this keyboard:

    make ogurec/left_pm:default:flash

To place the keyboard into bootloader mode, solder a reset switch onto the PCB and press it OR short the GND and RST pins on the pro micro. 

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
