# Quark_Squared

![Quark_Squared](https://i.imgur.com/zYH25zQ.png)

The Quark² PCB is a hotswap version of the Quark PCB. Just like the OG, it has a modified layout than a traditonal 4x12 and 5x12 ortholinear keyboard. 

* Keyboard Maintainer: [Nasp](https://github.com/npspears)
* Hardware Supported: Planck
* Hardware Availability: https://www.checkerboards.xyz/Quark2_p_35.html

Make example for this keyboard (after setting up your build environment):

    make checkerboards:quark_squared:default
    
These boards may be reset into bootloader either via the reset hardware button (on the back of the PCB near the USB connector) or through a configured RESET shortcut inserted into the keymap.     

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
