# CherryB Works CB65

![CB65](https://i.imgur.com/3qopFIWh.jpg)

An universal 65 percents PCB for many keyboard with USB daughterboard 
Board has a rotary encoder but disabled for VIA support.

* Keyboard Maintainer: lunaticwhat
* Hardware Supported: CB65, atmega32u4
* Hardware Availability: [CherryB Studio](https://discord.gg/qVwv3gcq83)

Make example for this keyboard (after setting up your build environment):

    make cherrybstudio/cb65:default

Flashing example for this keyboard:

    make cherrybstudio/cb65:default:flash

## Accessing Bootloader Mode

To access Bootloader Mode, do one of the following:

* Hold the top left key of the keyboard while connecting the USB cable

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
