# Andean Condor (andean_condor)

![Pic](https://i.imgur.com/woaDob6.jpg)

The Andean Condor is a monoblock split keyboard in the spirit of the Kyria.

* Keyboard Maintainer: [Guido Bartolucci](https://github.com/guidoism)
* Hardware Supported: Raspberry Pi Pico (only QMK), Nice!Nano (only ZMK)
* Hardware Availability: [Pico PCB](https://github.com/guidoism/andean-condor/tree/pico-w), [Nice!Nano PCB](https://github.com/guidoism/andean-condor)

Make example for this keyboard (after setting up your build environment):

    make andean_condor:default
    
or

    qmk compile -kb andean_condor -km default

Flashing example for this keyboard:

    make andean_condor:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader in 3 ways:

* **Bootmagic reset**: Hold down the key at (0,0) in the matrix (usually the top left key or Escape) and plug in the keyboard
* **Physical reset button**: Briefly press the button on the back of the PCB - some may have pads you must short instead
* **Keycode in layout**: Press the key mapped to `QK_BOOT` if it is available
&g
    
