# dumbpad v1.x with encoder on right side

![dumbpad](https://i.imgur.com/ND03FiFl.png)

A 4x4 numpad/macropad with a rotary encoder to the right of the bottom row of keys.

* Keyboard Maintainer: [imchipwood](https://github.com/imchipwood)
* Hardware repository: [dumbpad on github](https://github.com/imchipwood/dumbpad)
* PCB Revisions Supported: v1.0

Make example for this keyboard (after setting up your build environment):

    make dumbpad/v1x_right:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
