# Barleycorn SMD

![image](https://user-images.githubusercontent.com/3302524/110901245-a5679b00-82c9-11eb-8f8f-17ed6bd97332.png)

An f-row less compact 1800 keyboard with SMD components. Based on Barleycorn by Yiancar.

-   Keyboard Maintainer: matthewdias
-   Hardware Supported: Barleycorn SMD
-   Hardware Availability: https://p3dstore.com

Make example for this keyboard (after setting up your build environment):

    make barleycorn_smd:default

Flashing example for this keyboard:

    make barleycorn_smd:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
