flabbergast's TMK/ChibiOS port
==============================
2015/10/16


Build
-----
Set up ChibiOS according to tmk_core/protocol/chibios/README.md


Chibios Configuration
---------------------
halconf.h: for HAL configuration
    placed in project directory
    read in chibios/os/hal/hal.mk
    included in chibios/os/hal/include/hal.h
mcuconf.h: for MCU configuration
    placed in project directory
    included in halconf.h


Chibios Term
------------
PAL = Port Abstraction Layer
    palWritePad
    palReadPad
    palSetPad
    chibios/os/hal/include/pal.h

LLD = Low Level Driver


Makefile
--------
    #   <chibios>/os/hal/ports/$(MCU_FAMILY)/$(MCU_SERIES)
    MCU_FAMILY = KINETIS
    MCU_SERIES = KL2x

    # - it should exist either in <chibios>/os/common/ports/ARMCMx/compilers/GCC/ld/
    #   or <this_dir>/ld/
    MCU_LDSCRIPT = MKL26Z64

    #  - it should exist in <chibios>/os/common/ports/ARMCMx/compilers/GCC/mk/
    MCU_STARTUP = kl2x

    # Board: it should exist either in <chibios>/os/hal/boards/
    #  or <this_dir>/boards
    BOARD = PJRC_TEENSY_LC

    MCU  = cortex-m0

    # ARM version, CORTEX-M0/M1 are 6, CORTEX-M3/M4/M7 are 7
    ARMV = 6


halconf.h
---------


mcuconf.h
---------


chconf.h
--------


ld script
---------
--- ../../tmk_core/tool/chibios/chibios/os/common/ports/ARMCMx/compilers/GCC/ld/MKL26Z64.ld     2015-10-15 09:08:58.732904304 +0900
+++ ld/MKL26Z64.ld      2015-10-15 08:48:06.430215496 +0900
@@ -27,7 +27,8 @@
 {
   flash0   :  org = 0x00000000,  len = 0xc0
   flashcfg :  org = 0x00000400,  len = 0x10
-  flash    :  org = 0x00000410,  len = 64k - 0x410
+  flash    :  org = 0x00000410,  len = 62k - 0x410
+  eeprom_emu : org = 0x0000F800, len = 2k
   ram      :  org = 0x1FFFF800,  len = 8k
 }

@@ -35,6 +36,10 @@
 __ram_size__            = LENGTH(ram);
 __ram_end__             = __ram_start__ + __ram_size__;

+__eeprom_workarea_start__ = ORIGIN(eeprom_emu);
+__eeprom_workarea_size__  = LENGTH(eeprom_emu);
+__eeprom_workarea_end__   = __eeprom_workarea_start__ + __eeprom_workarea_size__;
+
 SECTIONS
 {
   . = 0;



Configuration/Startup for Infinity 60%
--------------------------------------
Configuration:


Clock:
Inifinity   
    FEI(FLL Engaged Internal) mode with core clock:48MHz, bus clock:48MHz, flash clock:24MHz
    Clock dividor:
    SIM_CLKDIV1[OUTDIV1] = 0 divide-by-1 for core clock
    SIM_CLKDIV1[OUTDIV2] = 0 divide-by-1 for bus clock
    SIM_CLKDIV1[OUTDIV4] = 1 divide-by-2 for flash clock
    Internal reference clock:
    MCG_C1[IREFS] = 1 Internal Reference Select for clock source for FLL
    MCG_C1[IRCLKEN] = 1 Internal Reference Clock Enable
    FLL multipilication:
    MCG_C4[DMX32] = 1
    MCG_C4[DRST_DRS] = 01   FLL factor 1464 * 32.768kHz = 48MHz

chibios/os/hal/ports/KINETIS/K20x/hal_lld.c
    k20x_clock_init(): called in __early_init() defined in board.c
        disable watchdog and configure clock

        configurable macros:
        KINETIS_NO_INIT: whether init or not
        KINETIS_MCG_MODE: clock mode   
            KINETIS_MCG_MODE_FEI
            KINETIS_MCG_MODE_PEE
                hal/ports/KINETIS/K20x/hal_lld.h
            

chibios/os/hal/boards/FREESCALE_FREEDOM_K20D50M/board.h
    PALConfig pal_default_config
    boardInit()
    __early_init()
    macro definitions for board infos, freq and mcu type

chibios/os/hal/boards/FREESCALE_FREEDOM_K20D50M/board.c

USB


Startup
-------
    common/ports/ARMCMx/GCC/crt0_v[67]m.s
        Reset_Handler: startup code
    common/ports/ARMCMx/GCC/crt1.c
        __core_init(): weak
        __early_init(): weak
        __late_init(): weak
        __default_exit(): weak
            called from Reset_Handler of crt0
    common/ports/ARMCMx/GCC/vector.c
    common/ports/ARMCMx/GCC/ld/*.ld

chibios/os/common/ports/ARMCMx/compilers/GCC/
├── crt0_v6m.s
├── crt0_v7m.s
├── crt1.c
├── ld
│   ├── MK20DX128BLDR3.ld
│   ├── MK20DX128BLDR4.ld
│   ├── MK20DX128.ld
│   ├── MK20DX256.ld
│   ├── MKL25Z128.ld
│   ├── MKL26Z128.ld
│   ├── MKL26Z64.ld
│   └── STM32L476xG.ld
├── mk
│   ├── startup_k20x5.mk
│   ├── startup_k20x7.mk
│   ├── startup_k20x.mk
│   ├── startup_kl2x.mk
│   └── startup_stm32l4xx.mk
├── rules.ld
├── rules.mk
└── vectors.c

chibios/os/hal/
├── boards
│   ├── FREESCALE_FREEDOM_K20D50M
│   │   ├── board.c
│   │   ├── board.h
│   │   └── board.mk
│   ├── MCHCK_K20
│   │   ├── board.c
│   │   ├── board.h
│   │   └── board.mk
│   ├── PJRC_TEENSY_3
│   │   ├── board.c
│   │   ├── board.h
│   │   └── board.mk
│   ├── PJRC_TEENSY_3_1
│   │   ├── board.c
│   │   ├── board.h
│   │   └── board.mk
│   ├── PJRC_TEENSY_LC
│   │   ├── board.c
│   │   ├── board.h
│   │   └── board.mk
│   ├── readme.txt
│   ├── simulator
│   │   ├── board.c
│   │   ├── board.h
│   │   └── board.mk
│   ├── ST_NUCLEO_F030R8
│   │   ├── board.c
│   │   ├── board.h
│   │   ├── board.mk
│   │   └── cfg
│   │       └── board.chcfg
├── hal.mk
├── include
│   ├── adc.h
│   ├── can.h
│   ├── dac.h
│   ├── ext.h
│   ├── gpt.h
│   ├── hal_channels.h
│   ├── hal_files.h
│   ├── hal.h
│   ├── hal_ioblock.h
│   ├── hal_mmcsd.h
│   ├── hal_queues.h
│   ├── hal_streams.h
│   ├── i2c.h
│   ├── i2s.h
│   ├── icu.h
│   ├── mac.h
│   ├── mii.h
│   ├── mmc_spi.h
│   ├── pal.h
│   ├── pwm.h
│   ├── rtc.h
│   ├── sdc.h
│   ├── serial.h
│   ├── serial_usb.h
│   ├── spi.h
│   ├── st.h
│   ├── uart.h
│   └── usb.h
├── lib
│   └── streams
│       ├── chprintf.c
│       ├── chprintf.h
│       ├── memstreams.c
│       ├── memstreams.h
│       ├── nullstreams.c
│       └── nullstreams.h
├── osal
│   ├── nil
│   │   ├── osal.c
│   │   ├── osal.h
│   │   └── osal.mk
│   ├── os-less
│   │   └── ARMCMx
│   │       ├── osal.c
│   │       ├── osal.h
│   │       └── osal.mk
│   └── rt
│       ├── osal.c
│       ├── osal.h
│       └── osal.mk
├── ports
│   ├── AVR
│   ├── common
│   │   └── ARMCMx
│   │       ├── mpu.h
│   │       ├── nvic.c
│   │       └── nvic.h
│   ├── KINETIS
│   │   ├── K20x
│   │   │   ├── hal_lld.c
│   │   │   ├── hal_lld.h
│   │   │   ├── kinetis_registry.h
│   │   │   ├── platform.dox
│   │   │   ├── platform.mk
│   │   │   ├── pwm_lld.c
│   │   │   ├── pwm_lld.h
│   │   │   ├── spi_lld.c
│   │   │   └── spi_lld.h
│   │   ├── KL2x
│   │   │   ├── hal_lld.c
│   │   │   ├── hal_lld.h
│   │   │   ├── kinetis_registry.h
│   │   │   ├── platform.mk
│   │   │   ├── pwm_lld.c
│   │   │   └── pwm_lld.h
│   │   ├── LLD
│   │   │   ├── adc_lld.c
│   │   │   ├── adc_lld.h
│   │   │   ├── ext_lld.c
│   │   │   ├── ext_lld.h
│   │   │   ├── gpt_lld.c
│   │   │   ├── gpt_lld.h
│   │   │   ├── i2c_lld.c
│   │   │   ├── i2c_lld.h
│   │   │   ├── pal_lld.c
│   │   │   ├── pal_lld.h
│   │   │   ├── serial_lld.c
│   │   │   ├── serial_lld.h
│   │   │   ├── st_lld.c
│   │   │   ├── st_lld.h
│   │   │   ├── usb_lld.c
│   │   │   └── usb_lld.h
│   │   └── README.md
│   ├── LPC
│   ├── simulator
│   └── STM32
├── src
│   ├── adc.c
│   ├── can.c
│   ├── dac.c
│   ├── ext.c
│   ├── gpt.c
│   ├── hal.c
│   ├── hal_mmcsd.c
│   ├── hal_queues.c
│   ├── i2c.c
│   ├── i2s.c
│   ├── icu.c
│   ├── mac.c
│   ├── mmc_spi.c
│   ├── pal.c
│   ├── pwm.c
│   ├── rtc.c
│   ├── sdc.c
│   ├── serial.c
│   ├── serial_usb.c
│   ├── spi.c
│   ├── st.c
│   ├── uart.c
│   └── usb.c
└── templates
    ├── adc_lld.c
    ├── adc_lld.h
    ├── can_lld.c
    ├── can_lld.h
    ├── dac_lld.c
    ├── dac_lld.h
    ├── ext_lld.c
    ├── ext_lld.h
    ├── gpt_lld.c
    ├── gpt_lld.h
    ├── halconf.h
    ├── hal_lld.c
    ├── hal_lld.h
    ├── i2c_lld.c
    ├── i2c_lld.h
    ├── i2s_lld.c
    ├── i2s_lld.h
    ├── icu_lld.c
    ├── icu_lld.h
    ├── mac_lld.c
    ├── mac_lld.h
    ├── mcuconf.h
    ├── osal
    │   ├── osal.c
    │   ├── osal.h
    │   └── osal.mk
    ├── pal_lld.c
    ├── pal_lld.h
    ├── platform.mk
    ├── pwm_lld.c
    ├── pwm_lld.h
    ├── rtc_lld.c
    ├── rtc_lld.h
    ├── sdc_lld.c
    ├── sdc_lld.h
    ├── serial_lld.c
    ├── serial_lld.h
    ├── spi_lld.c
    ├── spi_lld.h
    ├── st_lld.c
    ├── st_lld.h
    ├── uart_lld.c
    ├── uart_lld.h
    ├── usb_lld.c
    └── usb_lld.h
