# Record TCefTouchHandleState

Description
Fields

## Unit

uCEFTypes

## Declaration

`type TCefTouchHandleState = record`

## Description

Touch handle state.

<see href="https://bitbucket.org/chromiumembedded/cef/src/master/include/internal/cef_time.h">CEF source file: /include/internal/cef_time.h (cef_touch_handle_state_t))

## Overview

### Fields

Public | `size: NativeUInt;`
Public | `touch_handle_id: integer;`
Public | `flags: cardinal;`
Public | `enabled: integer;`
Public | `orientation: TCefHorizontalAlignment;`
Public | `mirror_vertical: integer;`
Public | `mirror_horizontal: integer;`
Public | `origin: TCefPoint;`
Public | `alpha: single;`

## Description

### Fields

Public | `size: NativeUInt;`
Size of this structure.

Public | `touch_handle_id: integer;`
Touch handle id. Increments for each new touch handle.

Public | `flags: cardinal;`
Combination of TCefTouchHandleStateFlags values indicating what state is set.

Public | `enabled: integer;`
Enabled state. Only set if |flags| contains CEF_THS_FLAG_ENABLED.

Public | `orientation: TCefHorizontalAlignment;`
Orientation state. Only set if |flags| contains CEF_THS_FLAG_ORIENTATION.

Public | `mirror_vertical: integer;`
This item has no description.

Public | `mirror_horizontal: integer;`
This item has no description.

Public | `origin: TCefPoint;`
Origin state. Only set if |flags| contains CEF_THS_FLAG_ORIGIN.

Public | `alpha: single;`
Alpha state. Only set if |flags| contains CEF_THS_FLAG_ALPHA.

Generated by PasDoc 1.0.4.