(footprint "CN800" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x12, 1.27mm pitch, single row")
  (tags "Through hole pin header THT 1x12 1.27mm single row")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr through_hole)
  (fp_text reference "CN800" (at 1.05 4.08 180) (layer "F.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold))
    (tstamp 4806d2ac-96fe-4aa6-a213-c5f576ba58ec)
  )
  (fp_text value "Conn_01x12" (at 0.05 5.96 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ec58a6a8-9ea0-4041-b33b-4b44b4a35a77)
  )
  (fp_text user "1" (at 8.2 2.26 unlocked) (layer "F.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold) (justify left bottom))
    (tstamp 97945b01-daf6-499c-9b1f-0214136c511e)
  )
  (fp_text user "12" (at -9.89 2.33 unlocked) (layer "F.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold) (justify left bottom))
    (tstamp c3d16eb4-c6c7-495e-aa0b-fbe3e59fd978)
  )
  (fp_text user "${REFERENCE}" (at 6.14 7.31 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 674ef515-4391-4690-886b-bd02d4ab7437)
  )
  (fp_line (start -6.4 -4.61) (end -6.4 -4.61)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp 4da9c671-2197-4c3e-99fd-08aae3094390))
  (fp_line (start -6.4 -4.61) (end -6.4 2.16)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp 0624027a-6534-4f6a-bac1-6f5ed242b26b))
  (fp_line (start -6.4 2.16) (end 7.54 2.16)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp 5e94b650-43a4-4203-8629-5fdf72231896))
  (fp_line (start 7.54 2.16) (end 7.54 -4.61)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp 9e4df69a-2662-4bf9-9001-7b6723ff067d))
  (pad "1" smd rect (at 5.98 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp 4f9c1c37-4031-4a55-ac7f-142ec41774dd))
  (pad "2" smd rect (at 4.98 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp 537a2d95-56ce-44c7-af85-fb36ef90e715))
  (pad "3" smd rect (at 3.98 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp b6150136-2d17-4755-9421-8357ab6726f8))
  (pad "4" smd rect (at 2.98 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp f458561a-87c1-40b7-bbf7-827ea53a97f7))
  (pad "5" smd rect (at 1.98 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp 9ec8e286-041c-4327-b358-fe235e38a9ab))
  (pad "6" smd rect (at 0.98 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp 4859cbbe-fd0e-4a26-941d-fff8fa877b8d))
  (pad "7" smd rect (at -0.02 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp 4ea7de80-fb64-4711-8170-e997ae2509b1))
  (pad "8" smd rect (at -1.02 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp 097a0ba4-eeb9-44c9-9214-d18be875855d))
  (pad "9" smd rect (at -2.02 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp dadf5149-a547-42a5-aa41-133f4210209b))
  (pad "10" smd rect (at -3.02 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp bd052433-1d6d-40d3-849d-5c6bb10d89ed))
  (pad "11" smd rect (at -4.02 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp 9278898b-65cd-4c46-80f1-96e7d43eea8d))
  (pad "12" smd rect (at -5.02 -0.31 180) (size 0.71 3.21) (layers "F.Cu" "F.Mask") (tstamp 934837a5-c759-4a93-9230-00eb770b5422))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x12_P1.27mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
