(footprint "Switch Type 2" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
  (tags "Through hole pin header THT 1x02 1.00mm single row")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Push button switch, generic, two pins")
  (property "ki_keywords" "switch normally-open pushbutton push-button")
  (attr through_hole)
  (fp_text reference "SW804" (at 0.4374 -9.870721) (layer "B.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold) (justify mirror))
    (tstamp 54d0fceb-e773-4f09-831d-6d123f6eac20)
  )
  (fp_text value "RUN" (at 0 2.56) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 682bff2a-040d-42aa-af18-2f4812d40da3)
  )
  (fp_text user "${REFERENCE}" (at 5 0.48 90) (layer "F.Fab")
      (effects (font (size 0.76 0.76) (thickness 0.114)))
    (tstamp 228d8d38-d18f-41de-af3a-bdab5db41348)
  )
  (pad "1" smd custom (at -2.29 -3.87) (size 2.18 2.18) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_line (start 0 0) (end 0.97 1.51) (width 0.7))
      (gr_arc (start 0.512825 6.033322) (mid 1.08 1.5) (end 5.051194 3.758831) (width 0.7))
      (gr_line (start 0.441007 1.981007) (end 2.34 3.88) (width 0.7))
      (gr_line (start 2.34 3.88) (end 2.34 3.88) (width 0.2))
      (gr_circle (center 2.34 3.88) (end 2.834975 3.88) (width 0.2) (fill yes))
    ) (tstamp 0e9f0d52-bad9-4eb8-9cc4-c8e206e69024))
  (pad "2" smd custom (at 2.28 3.91) (size 2.177119 2.177119) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_line (start 0 0) (end -1.55 -2.49) (width 0.7))
      (gr_arc (start -2.245806 -5.39) (mid -1.18218 -2.822181) (end -3.75 -3.885804) (width 0.7))
    ) (tstamp 36c4bd3d-b159-476f-ac03-893f8bc2e4e6))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
