(footprint "Resistor 0805 SMD" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
  (tags "resistor")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Resistor, small symbol")
  (property "ki_keywords" "R resistor")
  (attr smd)
  (fp_text reference "R800" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold))
    (tstamp 1ae4106e-b034-4ab5-8fc6-3eb450acae0d)
  )
  (fp_text value "R_Small" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 523a99e0-3074-45ca-aa89-96baed177537)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    (tstamp 3dc325fd-5a39-43f6-aeeb-bc2f5bcaa91c)
  )
  (fp_line (start -0.217064 -0.01) (end 0.237064 -0.01)
    (stroke (width 0.3) (type solid)) (layer "F.SilkS") (tstamp 9ba8e289-ad6c-4f80-a004-f2532fcf74ba))
  (fp_line (start -1.68 -0.95) (end 1.68 -0.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5f1b0fca-a347-49ad-b86f-7f3e9df6c79f))
  (fp_line (start -1.68 0.95) (end -1.68 -0.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a26f0e99-a796-4479-b13c-5feb534d1b0f))
  (fp_line (start 1.68 -0.95) (end 1.68 0.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3a36566d-6295-4c62-82e8-abc95c3a383f))
  (fp_line (start 1.68 0.95) (end -1.68 0.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ec25b330-032e-4cc9-a285-1148c9f7f9d3))
  (fp_line (start -1 -0.625) (end 1 -0.625)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fad9c936-12ac-4e30-8c1f-ed50f3c7d17f))
  (fp_line (start -1 0.625) (end -1 -0.625)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5be1b929-33df-4fb0-84f2-c7f9ca855d02))
  (fp_line (start 1 -0.625) (end 1 0.625)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 09997d6f-e3e8-4d69-a7b3-90e1080f89c3))
  (fp_line (start 1 0.625) (end -1 0.625)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 761d3a5a-b9da-40ad-b69c-97c94d29cfd7))
  (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902) (tstamp 0c1e88c3-78bf-4b27-8934-d07363001cd4))
  (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902) (tstamp 295795ef-ddcd-49aa-8b39-a5b694753d6f))
  (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
