(footprint "Ferrite" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
  (tags "resistor")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Ferrite bead, small symbol")
  (property "ki_keywords" "L ferrite bead inductor filter")
  (attr smd)
  (fp_text reference "L800" (at -2.56 -0.17 90) (layer "F.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold))
    (tstamp a50e7e6d-8c98-4286-a01b-a095dbace622)
  )
  (fp_text value "FerriteBead_Small" (at 1.66 -0.53 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4a8dafce-4301-4c25-a465-12d39abe1dfd)
  )
  (fp_text user "${REFERENCE}" (at 0.01 -0.53 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    (tstamp d55365ec-d55a-4165-8b40-4739023ef56f)
  )
  (fp_line (start 0.01 0.217064) (end 0.01 -0.237064)
    (stroke (width 0.3) (type solid)) (layer "F.SilkS") (tstamp eb445175-2247-4e90-8cba-0ed841ad2610))
  (fp_line (start -0.94 -2.21) (end 0.96 -2.21)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9013c75a-e9e9-4387-af97-455e8f0c684a))
  (fp_line (start -0.94 1.15) (end -0.94 -2.21)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8e671f47-da57-4d04-9939-788cb5c7e8ec))
  (fp_line (start 0.96 -2.21) (end 0.96 1.15)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bae1a579-5b9d-4510-bbd2-7defab588a22))
  (fp_line (start 0.96 1.15) (end -0.94 1.15)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dc9423f6-9461-4423-b3e8-24c99248d016))
  (fp_line (start -0.615 -1.53) (end 0.635 -1.53)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6f804009-cfca-432c-845f-778b609345af))
  (fp_line (start -0.615 0.47) (end -0.615 -1.53)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp efe3803f-c0b9-402b-8e7e-b8e28001ee1f))
  (fp_line (start 0.635 -1.53) (end 0.635 0.47)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d2c6ee37-5ea1-4209-b0a2-1388326d7f38))
  (fp_line (start 0.635 0.47) (end -0.615 0.47)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 86c3fc5d-8aa1-47a1-b48b-ab8c4191a55f))
  (pad "1" smd roundrect (at 0.054717 1.614717 90) (size 1.154417 1.854417) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902) (tstamp accf5676-b0c3-4f89-828d-17311e5acafa))
  (pad "2" smd roundrect (at 0.01 -1.44 90) (size 1.154417 1.854417) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902) (tstamp f86fac6a-e9dd-4ce0-ba29-6683655ac538))
  (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
