(footprint "CN801" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
  (tags "Through hole pin header THT 1x02 1.00mm single row")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr through_hole)
  (fp_text reference "CN801" (at 0 -1.56) (layer "B.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold) (justify mirror))
    (tstamp dcb0d819-ba2e-4687-95ba-33857cbc27a8)
  )
  (fp_text value "AUDIO" (at 0 2.56) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 25fdb507-dbec-4c0c-9e97-7a198053c8b7)
  )
  (fp_text user "${REFERENCE}" (at 4.2 0.68 90) (layer "F.Fab")
      (effects (font (size 0.76 0.76) (thickness 0.114)))
    (tstamp 0fe523f5-9b5f-4946-bf72-6d537f6d4c0e)
  )
  (fp_circle (center -1 0.840917) (end -0.59 1.110917)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 350f3ce2-428f-42d9-bd77-a37c69f69786))
  (fp_circle (center 1 0.840917) (end 1.41 1.110917)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp f353e924-2abe-423e-84c6-3cbc33ed4719))
  (pad "1" smd oval (at -1.04125 0.664334) (size 1.6425 2.715) (layers "F.Cu" "F.Mask") (tstamp 47d6a8b6-02fb-48e7-a760-90e2d82c059e))
  (pad "2" smd oval (at 1.04 0.664334) (size 1.6425 2.715) (layers "F.Cu" "F.Mask") (tstamp c4928c62-0f74-42a5-8b2d-9e7cfd1695b2))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
