(footprint "Diode SOT-23" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "SOT TO_SOT_SMD")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Dual 100V 215mA high-speed switching diodes, common cathode, SOT-23")
  (property "ki_keywords" "diode")
  (attr smd)
  (fp_text reference "D802" (at 0.16 3.1) (layer "F.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold))
    (tstamp c97dacf7-2e98-4687-9ecf-4025efc5da62)
  )
  (fp_text value "BAV70" (at 0 -2.39) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ec525560-b84a-4c57-a3dc-6633d57a7503)
  )
  (fp_text user "${REFERENCE}" (at 0 0.01) (layer "F.Fab")
      (effects (font (size 0.32 0.32) (thickness 0.05)))
    (tstamp eee78031-c76e-4bf7-af1e-897741be2113)
  )
  (fp_line (start -0.24 0) (end 0.19 0)
    (stroke (width 0.4) (type default)) (layer "F.SilkS") (tstamp 07d16174-d89b-4b12-a890-6057565748f6))
  (fp_line (start -1.92 -1.69) (end -1.92 1.71)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2929c9f8-6bdd-4c29-9ca0-0f55987831c9))
  (fp_line (start -1.92 1.71) (end 1.92 1.71)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 766e575f-1d82-4065-8f35-b3b62f23fbc1))
  (fp_line (start 1.92 -1.69) (end -1.92 -1.69)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 347f4a2f-bbf6-4476-9c63-5699a8b13a9b))
  (fp_line (start 1.92 1.71) (end 1.92 -1.69)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9f64c781-fae5-4a75-af08-170f36d3546a))
  (fp_line (start -0.65 -1.44) (end 0.65 -1.44)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8cae632f-8619-404d-8db2-cf232d386ea8))
  (fp_line (start -0.65 1.46) (end -0.65 -1.44)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 739599bc-c76d-44ca-a851-f547601de0fb))
  (fp_line (start 0.325 1.46) (end -0.65 1.46)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f6a4987b-1a02-44a6-b5cf-b209ab927e41))
  (fp_line (start 0.65 -1.44) (end 0.65 1.135)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6c8826e6-d81e-4254-9777-7ce664114dd0))
  (fp_line (start 0.65 1.135) (end 0.325 1.46)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c573f68e-a861-4cfe-9b95-3cd4ea6936d2))
  (pad "1" smd roundrect (at 1.1675 0.96 180) (size 1.015 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dc5fcba9-99b1-4bfc-b276-eeeba4b5cdfe))
  (pad "2" smd roundrect (at 1.1675 -0.94 180) (size 1.015 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f98c6ca6-d735-46e6-9f47-2c570e2f377d))
  (pad "3" smd roundrect (at -1.1325 0.01 180) (size 1.085 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 84affe80-b70a-425e-bfd6-d0b105dcdb98))
  (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
