(footprint "Turbo Switch" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x04 2.54mm single row")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Switch, three position, single pole triple throw, 3 position switch, SP3T")
  (property "ki_keywords" "switch sp3t ON-ON-ON")
  (attr through_hole)
  (fp_text reference "SW809" (at 0 -2.33) (layer "F.SilkS") hide
      (effects (font (size 1.3 1.3) (thickness 0.26) bold))
    (tstamp 6d8dfb28-d4f3-4a7f-a5cd-979852c6f87c)
  )
  (fp_text value "I TURBO" (at 0 9.95) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c23032d6-625c-4c1d-bf2c-00e3a71b94f2)
  )
  (fp_text user "${REFERENCE}" (at 5.79 3.25 270) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bcfff676-e74b-4e19-b214-108deb295d65)
  )
  (pad "1" smd rect (at -3.35 5.14) (size 3.25 2.15) (layers "F.Cu" "F.Mask") (tstamp d4757696-ed43-402b-b42d-df5c6dfeac5d))
  (pad "2" smd rect (at -0.065 5.14) (size 2.2 2.15) (layers "F.Cu" "F.Mask") (tstamp 6404dfce-dd92-44f2-b254-8edd5bd6c245))
  (pad "3" smd rect (at -0.0425 1.1625) (size 9.875 2.125) (layers "F.Cu" "F.Mask") (tstamp fada0ebe-6058-4c0a-ba2f-ddd8591e0f31))
  (pad "4" smd rect (at 3.225 5.14) (size 3.25 2.15) (layers "F.Cu" "F.Mask") (tstamp 8b07a18a-ff2e-4e8f-9648-b43db96c44e1))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
