(footprint "J800" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x05 2.54mm single row")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve")
  (property "ki_keywords" "audio jack receptacle mono phone headphone TS connector")
  (attr through_hole)
  (fp_text reference "J800" (at 0 -2.33) (layer "B.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold) (justify mirror))
    (tstamp 94f541ce-ce32-4303-884c-396e66e0f7dd)
  )
  (fp_text value "LINK" (at 0.04 3.39) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 141d5d8e-e769-4aed-81b7-e97947ae761b)
  )
  (fp_text user "${REFERENCE}" (at 0.06 5.17) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e019d119-36e9-471d-a4a0-964e68a185f7)
  )
  (fp_circle (center -0.02 0.79) (end 1.070413 0.79)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.Mask") (tstamp 499c799d-460a-4298-99ee-f7a3b616f3c2))
  (fp_rect (start -5.41 -0.02) (end -4.6 1.61)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp da1b44de-ae08-450a-9ed8-0bf4f0a163f0))
  (fp_rect (start -2.98 -0.02) (end -2.17 1.61)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 7724f59a-9099-4db1-872e-b045fcabcd62))
  (fp_rect (start 1.97 -0.02) (end 2.78 1.61)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp e31d06ef-c60e-4d2a-a716-895c6cc7de17))
  (fp_rect (start 4.52 -0.02) (end 5.33 1.61)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 52ccae70-c3d5-41d9-bfd3-c6c280ebacf1))
  (fp_circle (center -0.042681 0.78) (end 0.627319 0.84)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 6d236921-a653-49e3-b2a4-2b3c2e8c080a))
  (pad "G" smd oval (at -2.48 0.4975) (size 2.165 3.685) (layers "F.Cu" "F.Mask") (tstamp bce56e07-672a-4431-a96d-16fdf9377afd))
  (pad "G" smd oval (at 2.46 0.4975) (size 2.165 3.685) (layers "F.Cu" "F.Mask") (tstamp 557263f8-873b-40f5-b364-a0b6cbefc928))
  (pad "S" smd oval (at -5.0125 0.4975) (size 2.165 3.685) (layers "F.Cu" "F.Mask") (tstamp 03b1e7d5-c3de-463c-a0bd-f1ae816b6d51))
  (pad "T" smd oval (at 4.96 0.4975) (size 2.165 3.685) (layers "F.Cu" "F.Mask") (tstamp 4b269564-0c40-4b61-bce7-84474e18ac47))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
