(footprint "IC800" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT358-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "LQFP QFP")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "UIC800" (at -8.6 5.68 180) (layer "F.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold))
    (tstamp c1dc44cf-2585-466b-8316-d5b265d05d53)
  )
  (fp_text value "BU5782K" (at -0.17 5.64 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d7eac66e-1b36-4ce4-947e-bf2405b0efaa)
  )
  (fp_text user "${REFERENCE}" (at -0.17 -0.24 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8bc78115-b779-4fa5-a4b8-0929a3d9dd66)
  )
  (fp_line (start -3.335 -1.985) (end -1.825 -3.495)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp 59257db7-7763-47ea-a109-b98a1d2ee5f5))
  (fp_rect (start -3.35 -3.51) (end 3.4 3.24)
    (stroke (width 0.25) (type default)) (fill none) (layer "F.SilkS") (tstamp 3dca18cc-791f-44c7-a3ef-2f2c8ed3412b))
  (fp_line (start -5.35 -3.54) (end -5.35 -0.24)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6f86a50e-0054-485a-a851-8aa8ad8eb4eb))
  (fp_line (start -5.35 3.06) (end -5.35 -0.24)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8194e184-a3b5-46c9-ab38-c7b01fe81921))
  (fp_line (start -3.92 -3.99) (end -3.92 -3.54)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ed60bf4a-aa11-4abe-80a7-848d2437d3c9))
  (fp_line (start -3.92 -3.54) (end -5.35 -3.54)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8c26d534-722c-4cad-a5f6-5b709b906cf8))
  (fp_line (start -3.92 3.06) (end -5.35 3.06)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4eadea6f-0104-4d92-b271-1255415df1fe))
  (fp_line (start -3.92 3.51) (end -3.92 3.06)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 96f4d87a-c24f-4661-a1a0-7077378e661d))
  (fp_line (start -3.47 -5.42) (end -3.47 -3.99)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 450fa49a-7383-43cf-bed5-45c7ca8a228e))
  (fp_line (start -3.47 -3.99) (end -3.92 -3.99)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 671f208d-0d83-4b46-83b5-ef2dbc7d8499))
  (fp_line (start -3.47 3.51) (end -3.92 3.51)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 48c2e83a-c245-42ab-9014-1c778b4ccc11))
  (fp_line (start -3.47 4.94) (end -3.47 3.51)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 788b11f8-4fd3-45e9-9a2b-92f42a1f51c0))
  (fp_line (start -0.17 -5.42) (end -3.47 -5.42)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d24d9d37-d2ac-4102-8f8d-c5143b9a313c))
  (fp_line (start -0.17 -5.42) (end 3.13 -5.42)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5f216d31-ee47-4e7b-a70f-a4f72ef7ae28))
  (fp_line (start -0.17 4.94) (end -3.47 4.94)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 51c20af8-2898-4795-8fbb-2c8ea6528e61))
  (fp_line (start -0.17 4.94) (end 3.13 4.94)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 805c1325-50d5-4d92-b927-211cf8da725a))
  (fp_line (start 3.13 -5.42) (end 3.13 -3.99)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 07138540-fc52-476c-b62b-e299aff8c2ba))
  (fp_line (start 3.13 -3.99) (end 3.58 -3.99)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7c69c88c-0a26-44e8-bf50-bdbccaa50b9c))
  (fp_line (start 3.13 3.51) (end 3.58 3.51)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f180f3ad-2471-4be1-9260-c7ef17bfee23))
  (fp_line (start 3.13 4.94) (end 3.13 3.51)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4bf32070-384a-4d27-b7fa-d37f06830543))
  (fp_line (start 3.58 -3.99) (end 3.58 -3.54)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 14640696-5b94-49b4-a5f0-8a2a2b306f40))
  (fp_line (start 3.58 -3.54) (end 5.01 -3.54)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2a823ff3-122b-42c6-9bcb-93b8d489235b))
  (fp_line (start 3.58 3.06) (end 5.01 3.06)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 881599ce-207b-42f3-a277-60c2cfc57cea))
  (fp_line (start 3.58 3.51) (end 3.58 3.06)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4e1f8f3b-3c6b-426e-bad6-44baf36436e4))
  (fp_line (start 5.01 -3.54) (end 5.01 -0.24)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a1be3111-d7aa-4aa6-afe7-c6ca3aaab0e5))
  (fp_line (start 5.01 3.06) (end 5.01 -0.24)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4ef21a6b-61af-4b9c-a700-208ba4aaa9f1))
  (fp_line (start -3.67 -2.74) (end -2.67 -3.74)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 07575b0b-2e45-4296-a942-da6fc54548bd))
  (fp_line (start -3.67 3.26) (end -3.67 -2.74)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8190eb8c-2d10-4b85-8e0c-c2929990a8fe))
  (fp_line (start -2.67 -3.74) (end 3.33 -3.74)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6c5cb490-8cf4-4f8a-b556-ccce9dccfa08))
  (fp_line (start 3.33 -3.74) (end 3.33 3.26)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 98a4ebe0-bf8b-4db4-bca6-6fc76b5292e4))
  (fp_line (start 3.33 3.26) (end -3.67 3.26)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4a8db27b-a298-429b-b484-bfada67aebc7))
  (pad "1" smd roundrect (at -4.345 -3.04) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d3cc5016-0bc1-48e6-aed4-6189d747e51e))
  (pad "2" smd roundrect (at -4.345 -2.24) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7a3803f2-9eef-4d96-8036-fe6ac7b41af4))
  (pad "3" smd roundrect (at -4.345 -1.44) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ad1cf93d-0905-49c8-863d-32f77bc2b3a0))
  (pad "4" smd roundrect (at -4.345 -0.64) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c0e7ec49-f35a-4bce-8def-e6e10dc24840))
  (pad "5" smd roundrect (at -4.345 0.16) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b2bbcf1c-6803-44c6-9568-841f1602c156))
  (pad "6" smd roundrect (at -4.345 0.96) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b7553011-330b-49cb-8dd1-0310304ae413))
  (pad "7" smd roundrect (at -4.345 1.76) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 09e83646-f745-4813-bb72-f9561075ff32))
  (pad "8" smd roundrect (at -4.345 2.56) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b863ade0-3f15-434c-bb64-24ded6483618))
  (pad "9" smd roundrect (at -2.9 4.17) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6c9e81be-b4c9-4846-a465-ad01f7705a43))
  (pad "10" smd roundrect (at -2.1 4.17) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e5e56268-fb2c-4876-9f98-357da0152c9e))
  (pad "11" smd roundrect (at -1.3 4.17) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2c9d1046-fc1f-429f-9fa5-a9bc539f5d74))
  (pad "12" smd roundrect (at -0.5 4.17) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 06a9bfd5-0e60-4f37-a0c6-89ff05d76a8c))
  (pad "13" smd roundrect (at 0.3 4.17) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 90a8a566-14a8-4c16-a017-970f5edbf627))
  (pad "14" smd roundrect (at 1.1 4.17) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 17e716ce-1221-4302-b0e2-b27f10fd6b90))
  (pad "15" smd roundrect (at 1.9 4.17) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bc4e9ca0-d13e-47a7-a06f-a9f2374d30c3))
  (pad "16" smd roundrect (at 2.7 4.17) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5f73f251-649e-4c05-8df4-d38fe58de98d))
  (pad "17" smd roundrect (at 4.43 2.56) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7f64b553-5ac8-4009-b59e-59174d650812))
  (pad "18" smd roundrect (at 4.43 1.76) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a81aa008-8a53-41d7-9880-b11845056d90))
  (pad "19" smd roundrect (at 4.43 0.96) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 687b20f1-5d3b-463d-a323-adf259d48ead))
  (pad "20" smd roundrect (at 4.43 0.16) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2eb1572f-f7ab-4d26-8830-2e45d70a4d34))
  (pad "21" smd roundrect (at 4.43 -0.64) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1edfee17-f62b-40ce-a144-a663bf1b637c))
  (pad "22" smd roundrect (at 4.43 -1.44) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3a530d4c-2ce7-44ae-86f8-c58c796142c1))
  (pad "23" smd roundrect (at 4.43 -2.24) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 19d46d57-dbbb-4ce4-853c-c03a6517cf97))
  (pad "24" smd roundrect (at 4.43 -3.04) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fa503179-adca-45eb-9291-be353fdb29a1))
  (pad "25" smd roundrect (at 2.7 -4.43) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp edf4efbc-ba79-4ca2-bb12-181d4d64a0fb))
  (pad "26" smd roundrect (at 1.9 -4.43) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 61ae6d41-04ca-43d9-8879-8333a4e39960))
  (pad "27" smd roundrect (at 1.1 -4.43) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp de463765-ab72-4b73-8b03-0357a3e6358f))
  (pad "28" smd roundrect (at 0.3 -4.43) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5aac07ad-0bea-4efa-8c8a-d6190dc9f7db))
  (pad "29" smd roundrect (at -0.5 -4.43) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 628efb2a-fac3-4270-a0d1-6114f280a462))
  (pad "30" smd roundrect (at -1.3 -4.43) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4f5c4111-bb20-4501-9296-b9a4949ff524))
  (pad "31" smd roundrect (at -2.1 -4.43) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7caf9c01-0227-4715-8178-c5fbe07c18bb))
  (pad "32" smd roundrect (at -2.9 -4.43) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5538ac4f-e372-49d4-ad46-f6ffd4da60d0))
  (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-32_7x7mm_P0.8mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
