(footprint "Switch Type 5" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
  (tags "Through hole pin header THT 1x02 1.00mm single row")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Push button switch, generic, two pins")
  (property "ki_keywords" "switch normally-open pushbutton push-button")
  (attr through_hole)
  (fp_text reference "SW805" (at -9.3105 2.224) (layer "B.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold) (justify mirror))
    (tstamp beda7140-af22-48fb-8913-572a5ceccaa9)
  )
  (fp_text value "UP" (at 0 2.56) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 213b2d60-ea80-4366-a423-ef14bf98e787)
  )
  (fp_text user "${REFERENCE}" (at 0 0.5 90) (layer "F.Fab")
      (effects (font (size 0.76 0.76) (thickness 0.114)))
    (tstamp ad8ea464-40bf-4b57-a1f1-2f12f4790ce3)
  )
  (fp_line (start -1.15 -1) (end -1.15 2)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2dacaff0-5c65-418b-9884-0c5669121d03))
  (fp_line (start -1.15 2) (end 1.15 2)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b3df7d6c-31bd-4a9f-a223-02957b8ea1c1))
  (fp_line (start 1.15 -1) (end -1.15 -1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dbe19c5f-e83f-4ca0-9978-10369bd296b9))
  (fp_line (start 1.15 2) (end 1.15 -1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7d5e24b6-cc1e-48ab-8f87-ee777f88e727))
  (fp_line (start -0.635 -0.1825) (end -0.3175 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e335d250-b451-4ae3-a3b2-89546490c892))
  (fp_line (start -0.635 1.5) (end -0.635 -0.1825)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c2e16d66-1efd-4a99-bab3-ac1a43fb2e34))
  (fp_line (start -0.3175 -0.5) (end 0.635 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f49014b4-0c46-42f5-ae3b-9cec8319102a))
  (fp_line (start 0.635 -0.5) (end 0.635 1.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f9a7db4-ed83-49da-84aa-13ab8b59899e))
  (fp_line (start 0.635 1.5) (end -0.635 1.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0bc32796-d487-4009-8e0d-5478fd8b2212))
  (pad "1" smd custom (at -2.01 -1.54 90) (size 2.665 3.345) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_rect (start -1.2425 1.6725) (end -0.1975 2.7325) (width 0.2) (fill yes))
      (gr_rect (start -1.2425 2.6725) (end 1.2325 5.8325) (width 0.2) (fill yes))
      (gr_circle (center 1.4645 6.06) (end 2.689 6.06) (width 0.2) (fill yes))
    ) (tstamp 9175ac85-7eb4-4ebb-944d-c1b676c4d8da))
  (pad "2" smd custom (at 2.24 1.56 270) (size 2.665 3.345) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_rect (start -1.2425 1.6725) (end -0.1975 2.7325) (width 0.2) (fill yes))
      (gr_rect (start -1.2425 2.6725) (end 1.2325 5.8325) (width 0.2) (fill yes))
      (gr_circle (center 1.4645 6.06) (end 2.689 6.06) (width 0.2) (fill yes))
    ) (tstamp 8e180d7f-a86e-44f3-80c0-a6f6bb103b4f))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
