(footprint "Switch Type 3" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
  (tags "Through hole pin header THT 1x02 1.00mm single row")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Push button switch, generic, two pins")
  (property "ki_keywords" "switch normally-open pushbutton push-button")
  (attr through_hole)
  (fp_text reference "SW802" (at 0.4374 -9.870721) (layer "B.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold) (justify mirror))
    (tstamp 2ba4aeac-fbfc-4d07-b76c-86ecb0bd745b)
  )
  (fp_text value "II" (at 0 2.56) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 11a7a867-1ff4-4c5c-8f8b-9d43c2c2b753)
  )
  (fp_text user "${REFERENCE}" (at 5 0.48 90) (layer "F.Fab")
      (effects (font (size 0.76 0.76) (thickness 0.114)))
    (tstamp 3aabdba2-a16d-4f13-8af8-77dffdc5d5ba)
  )
  (pad "1" smd custom (at -5.17 -2.64) (size 2.18 2.18) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_line (start 0 0) (end 2.48 -1.25) (width 0.7))
      (gr_arc (start 3.342825 0.113322) (mid 3.91 -4.42) (end 7.881194 -2.161169) (width 0.7))
      (gr_line (start 3.271007 -3.938993) (end 5.17 -2.04) (width 0.7))
      (gr_circle (center 5.17 -2.04) (end 5.664975 -2.04) (width 0.2) (fill yes))
      (gr_line (start 5.17 -2.04) (end 5.17 -2.04) (width 0.2))
    ) (tstamp b61420b2-d778-4575-9e4c-292927f76dd0))
  (pad "2" smd custom (at 2.23 -0.78) (size 2.177119 2.177119) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_line (start 0 0) (end -1.55 -2.49) (width 0.7))
      (gr_arc (start -2.245806 -5.39) (mid -1.18218 -2.822181) (end -3.75 -3.885804) (width 0.7))
    ) (tstamp c411eac7-1380-45c4-95d1-0b45f3140aac))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
