(footprint "CC800 Electrolytic" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
  (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
  (property "Sheetfile" "pce-gt-controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Polarized capacitor, small symbol")
  (property "ki_keywords" "cap capacitor")
  (attr through_hole)
  (fp_text reference "CC800" (at 1.25 -3.75) (layer "B.SilkS")
      (effects (font (size 1.3 1.3) (thickness 0.26) bold) (justify mirror))
    (tstamp 80708695-ff75-4ed3-97d3-34656ded82b6)
  )
  (fp_text value "47uF 6.3v" (at 1.25 3.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c7f19b8c-45d9-41d7-9bcc-d3e0f52a8e7a)
  )
  (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8a436764-5d46-4d7a-b015-d7227114e84e)
  )
  (fp_circle (center -0.01 0) (end 0.27 0.28)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 81a5965a-938e-4c75-9629-57242827dc1a))
  (fp_circle (center 2.484021 0) (end 2.764021 0.28)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 7cde3e57-5ea4-4ce2-bde4-f60e276e2789))
  (fp_circle (center 1.25 0) (end 4 0)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp db478fe7-3acb-4fbb-8d92-bb18314232a7))
  (fp_line (start -0.883605 -1.0875) (end -0.383605 -1.0875)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5df90f38-2e2a-438d-9fc5-21da75af2bf2))
  (fp_line (start -0.633605 -1.3375) (end -0.633605 -0.8375)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e84e7e15-248c-497d-b60c-3667264cbb68))
  (fp_circle (center 1.25 0) (end 3.75 0)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 4ae98dd9-1ee7-4055-9f3e-f5b13936b5f5))
  (pad "1" smd circle (at 0 0) (size 1.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 307cfa0e-2209-4be8-9092-90884ea4414c))
  (pad "2" smd circle (at 2.494021 0) (size 1.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f9c190a2-4adb-4527-b75e-71ee5abd85bf))
  (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
