/*--------------------------------*- C++ -*----------------------------------*\
Volume-averaged temperature of the ablative material (gas + solid).
Please activate the right boundaryField for the 'top' Patch.
In other words, place the '/*' in front of the wrong 'top' option.
\*---------------------------------------------------------------------------*/
FoamFile {
  version     2.0;
  format      ascii;
  class       volScalarField;
  object      Ta;
}
// * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * //

dimensions      [0 0 0 1 0 0 0];

internalField   uniform 300;

boundaryField {
  porousMat_to_demiseMat
  {
    type            compressible::turbulentTemperatureCoupledBaffleMixed;
    value           uniform 310;
    Tnbr 		Ta;
    kappaMethod     lookup;
    kappa           k_abl_sym;
  }

  bottom
  {
    type            zeroGradient;
  }
  top
  {
    type            zeroGradient;
  }
  lateral
  {
    type            zeroGradient;
  }

  wedge_pos
  {
    type            wedge;
  }

  wedge_neg
  {
    type            wedge;
  }

  center
  {
    type            empty;
  }

}

// ************************************************************************* /
