/*--------------------------------*- C++ -*----------------------------------*\
Volume-averaged temperature of the ablative material (gas + solid).
Please activate the right boundaryField for the 'top' Patch.
In other words, place the '/*' in front of the wrong 'top' option.
\*---------------------------------------------------------------------------*/
FoamFile {
  version     2.0;
  format      ascii;
  class       volScalarField;
  object      Ta;
}
// * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * //

dimensions      [0 0 0 1 0 0 0];

internalField   uniform 300;

boundaryField {
  top
  {
    type        boundaryMapping;
    mappingType constant;
    mappingFileName "constant/porousMat/BoundaryConditions";
    mappingFields
    (
        (Ta "2")
    );
    value           uniform 300;
  }
  sides
  {
    type		empty;
  }
  wedge_pos
  {
    type            wedge;
  }
  wedge_neg
  {
    type            wedge;
  }
  center
  {
    type		empty;
  }

}
// ************************************************************************* /
