# KDA kernel implementation with TileLang
## Requirement
- TileLang: 0.1.6.post2+cuda.git729e66ca
- triton: 3.2.0
- FLA: commit 9714c5(used for comparison)

We copy the needed files and function from flash-linear-attention to the FLA_KDA/ for easily comparison.
