# Sample NVRAM for BCM94339 WLCSP with eTR,iPA, and eLNA.
sromrev=11
boardrev=0x1100
boardtype=0x06c9
boardflags=0x10081401
boardflags2=0x00000000
boardflags3=0x08001188
#boardnum=57410
macaddr=00:90:4c:c5:12:38
ccode=0
regrev=0
antswitch=0
pdgain2g=7
pdgain5g=7
tworangetssi2g=0
tworangetssi5g=0
vendid=0x14e4
devid=0x43ae
manfid=0x2d0
#prodid=0x052e
nocrc=1
otpimagesize=502
xtalfreq=37400
extpagain2g=2
pdetrange2g=2
extpagain5g=2
pdetrange5g=2
rxgains2gelnagaina0=2
rxgains2gtrisoa0=6
rxgains2gtrelnabypa0=1
rxgains5gelnagaina0=4
rxgains5gtrisoa0=4
rxgains5gtrelnabypa0=1
rxchain=1
txchain=1
aa2g=1
aa5g=1
tssipos5g=0
tssipos2g=0
pa2ga0=0xFF47,0x17B5,0xFD2B
pa2gccka0=0xFF5F,0x1B46,0xFCCC
pa5ga0=0xff54,0x16ec,0xfd45,0xff52,0x16a1,0xfd4d,0xff46,0x15b7,0xfd5a,0xff56,0x156d,0xfd79
pa5gbw40a0=0xff59,0x17ca,0xfd30,0xff42,0x163d,0xfd4b,0xff31,0x152e,0xfd55,0xff60,0x16d8,0xfd54
pa5gbw80a0=0xff56,0x1740,0xfd3f,0xff50,0x1738,0xfd3d,0xff4d,0x16b4,0xfd42,0xff58,0x1634,0xfd60
# Default Target Power for 2G -- 17dBm(11)/14dBm(54)/13dBm(MCS7)/12dBm(MCS8)/12dBm(MCS9)
maxp2ga0=74
maxp5ga0=74,74,74,74
cckbw202gpo=0x0000
cckbw20ul2gpo=0x0000
mcsbw202gpo=0xaa888888
mcsbw402gpo=0xaa888888
dot11agofdmhrbw202gpo=0x6666
ofdmlrbw202gpo=0x0066
tssifloor2g=500
# Default Target Power for 5G -- 14dBm(54)/13dBm(MCS7)/12dBm(MCS8)/12dBm(MCS9)
mcsbw205glpo=0xaa866666
mcsbw405glpo=0xaa866666
mcsbw805glpo=0xaa866666
mcsbw205gmpo=0xaa866666
mcsbw405gmpo=0xaa866666
mcsbw805gmpo=0xaa866666
mcsbw205ghpo=0xaa866666
mcsbw405ghpo=0xaa866666
mcsbw805ghpo=0xaa866666
mcslr5glpo=0x0000
mcslr5gmpo=0x0000
mcslr5ghpo=0x0000
sb20in40hrpo=0x0
sb20in80and160hr5glpo=0x0
sb40and80hr5glpo=0x0
sb20in80and160hr5gmpo=0x0
sb40and80hr5gmpo=0x0
sb20in80and160hr5ghpo=0x0
sb40and80hr5ghpo=0x0
sb20in40lrpo=0x0
sb20in80and160lr5glpo=0x0
sb40and80lr5glpo=0x0
sb20in80and160lr5gmpo=0x0
sb40and80lr5gmpo=0x0
sb20in80and160lr5ghpo=0x0
sb40and80lr5ghpo=0x0
dot11agduphrpo=0x0
dot11agduplrpo=0x0
phycal_tempdelta=25
cckdigfilttype=2
swctrlmap_5g=0x00080008,0x00500010,0x00100008,0x000000,0x078
swctrlmap_2g=0x00010001,0x00220002,0x00020001,0x042202,0x1ff
swctrlmapext_5g=0x00000000,0x00000000,0x00000000,0x000000,0x000
swctrlmapext_2g=0x00000000,0x00000000,0x00000000,0x000000,0x000
#
#GPIO 0 for SDIO HW OOB interruption
#muxenab=0x10
#sd_gpout=0
#sd_oobonly=1
#
rssicorrnorm_c0=-2,0
rssicorrnorm5g_c0=3,5,2,3,4,2,2,3,1,2,3,1
## ED threshold level to address the new ETSI requirement - 10/31/2013
ed_thresh2g=-77
ed_thresh5g=-77
#
paparambwver=1
