TOPICS
------
    * INSTALLATION
    * GHOSTSCRIPT BUGS
    * FEDORA NOTES 
    * UBUNTU NOTES
    * DEBIAN NOTES
    * OPENSUSE 1x.x NOTES
    * ACER ASPIRE ONE NOTES
    * ASUS EEE PC NOTES
    * MAC OS X NOTES
    * FREEBSD NOTES
    * OPENBSD NOTES
    * OPENSOLARIS, SOLARIS EXPRESS DEVELOPER EDITION 9/07, Solaris 11+ NOTES
    * MINOLTA-QMS 2200/2300 DL NOTES
    * CUPS USB NOTES
    * HP LASERJET 1000/1005/1018/1020, P1005/P1006/P1007/P1008/P1505 NOTES
    * HP SMART INSTALL NOTES
    * PSUTILS AND 2/4-UP CAPABILITY
    * CUSTOM PAGE SIZE
    * LANDSCAPE ORIENTATION
    * SET DEFAULT MEDIA WITH CUPS
    * MANUAL DUPLEX
    * UPDATE
    * UNINSTALLING
    * BUG REPORTS
    * DEVELOPER AND DEBUGGING TIPS
    * CUSTOM ICC/ICM COLOR PRINTER PROFILE (BUY)
    * CUSTOM ICC/ICM COLOR PRINTER PROFILE (ARGYLL)

INSTALLATION
------------
Unpack:
    $ wget -O foo2zjs.tar.gz http://foo2zjs.rkkda.com/foo2zjs.tar.gz
    $ tar zxf foo2zjs.tar.gz
    $ cd foo2zjs

(Optional) Uninstall:
    $ su		OR	$ sudo make uninstall
    # make uninstall

Compile:
    $ make

Get extra files from the web, such as .ICM profiles (for color correction)
and firmware.  Select the model number for your printer:
    $ ./getweb 1025     # Get HP LaserJet Pro CP1025nw .ICM files
    $ ./getweb 1215	# Get HP Color LaserJet CP1215 .ICM files
    $ ./getweb 1500	# Get HP Color LaserJet 1500 .ICM files
    $ ./getweb 1600	# Get HP Color LaserJet 1600 .ICM files
    $ ./getweb 2600n	# Get HP Color LaserJet 2600n .ICM files

    $ ./getweb 1600w    # Get Konica Minolta magicolor 1600W .ICM files
    $ ./getweb 1680     # Get Konica Minolta magicolor 1680MF .ICM files
    $ ./getweb 1690     # Get Konica Minolta magicolor 1690MF .ICM files
    $ ./getweb 2480	# Get Konica Minolta magicolor 2480 MF .ICM files
    $ ./getweb 2490	# Get Konica Minolta magicolor 2490 MF .ICM files
    $ ./getweb 2530	# Get Konica Minolta magicolor 2530 DL .ICM files
    $ ./getweb 4690     # Get Konica Minolta magicolor 4690MF .ICM files
    $ ./getweb 110      # Get Oki C110 .ICM files
    $ ./getweb 6115	# Get Xerox Phaser 6115MFP .ICM files
    $ ./getweb 6121     # Get Xerox Phaser 6121MFP.ICM files

    $ ./getweb cpwl	# Get Minolta Color PageWorks/Pro L .ICM files
    $ ./getweb 2200	# Get Minolta/QMS magicolor 2200 DL .ICM files
    $ ./getweb 2300	# Get Minolta/QMS magicolor 2300 DL .ICM files
    $ ./getweb 2430	# Get Konica Minolta magicolor 2430 DL .ICM files

    $ ./getweb 300      # Get Samsung CLP-300 .ICM files
    $ ./getweb 315      # Get Samsung CLP-315 .ICM files
    $ ./getweb 325      # Get Samsung CLP-325 .ICM files
    $ ./getweb 360      # Get Samsung CLP-360 .ICM files
    $ ./getweb 365      # Get Samsung CLP-365 .ICM files
    $ ./getweb 600      # Get Samsung CLP-600 .ICM files
    $ ./getweb 610      # Get Samsung CLP-610 .ICM files
    $ ./getweb 2160     # Get Samsung CLX-2160 .ICM files
    $ ./getweb 3160     # Get Samsung CLX-3160 .ICM files
    $ ./getweb 3175     # Get Samsung CLX-3175 .ICM files
    $ ./getweb 3185     # Get Samsung CLX-3185 .ICM files
    $ ./getweb 6110     # Get Xerox Phaser 6110 and 6110MFP .ICM files

    $ ./getweb 500      # Get Lexmark C500 .ICM files

    $ ./getweb 301      # Get Oki C301dn .ICM files
    $ ./getweb c310     # Get Oki C310dn .ICM files
    $ ./getweb c511     # Get Oki C511dn .ICM files
    $ ./getweb c810     # Get Oki C810 .ICM files
    $ ./getweb 3200     # Get Oki C3200 .ICM files
    $ ./getweb 3300     # Get Oki C3300 .ICM files
    $ ./getweb 3400     # Get Oki C3400 .ICM files
    $ ./getweb 3530     # Get Oki C3530 MFP .ICM files
    $ ./getweb 5100     # Get Oki C5100 .ICM files
    $ ./getweb 5200     # Get Oki C5200 .ICM files
    $ ./getweb 5500     # Get Oki C5500 .ICM files
    $ ./getweb 5600     # Get Oki C5600 .ICM files
    $ ./getweb 5800     # Get Oki C5800 .ICM files

    $ ./getweb 160	# Get Olivetti d-Color P160W .ICM files

    $ ./getweb 1000	# Get HP LaserJet 1000 firmware file
    $ ./getweb 1005	# Get HP LaserJet 1005 firmware file
    $ ./getweb 1018	# Get HP LaserJet 1018 firmware file
    $ ./getweb 1020	# Get HP LaserJet 1020 firmware file

    $ ./getweb P1005	# Get HP LaserJet P1005 firmware file
    $ ./getweb P1006	# Get HP LaserJet P1006 firmware file
    $ ./getweb P1007	# Get HP LaserJet P1007 firmware file
    $ ./getweb P1008	# Get HP LaserJet P1008 firmware file
    $ ./getweb P1505	# Get HP LaserJet P1505 firmware file

Install driver, foomatic XML files, PPD files, and extra files:
    $ su		OR	$ sudo make install
    # make install

(Optional) Install hotplug (for HP LJ 1000/1005/1018/1020/P100[5678]/P1505):
    $ su		OR	$ sudo make install-hotplug
    # make install-hotplug

    Unplug and re-plug the USB printer

If you use CUPS to manage your printers, you must restart cupsd:
    # make cups		OR	$ sudo make cups

Test operation of programs. Skip this if you don't have the exact same
version of Ghostscript that I have, Fedora ghostscript 8.71-16.fc14, because
it will not pass since different versions of Ghostscript generate different
raster images:
    # make test

Create printers (Fedora 6/7/8/.../16 and Ubuntu 7.10/8.x/9.x/10.x/11.x):
    # system-config-printer

Create printers (Redhat 7.2/7.3/8.0/9.0, Fedora Core 1-5):
    # printconf-gui

Create printers (Mandrake/Manrivia)
    # printerdrake

Create printers (openSUSE 10.x/11.x)
    # yast2 printer

Create printers (Ubuntu 5.10/6.06/6.10/7.04)
    $ sudo gnome-cups-manager
    $ sudo make cups		# Ubuntu has a bug in gnome-cups-manager

	NOTE: to edit a queue hit "Properties" (click right mouse button).

Create printers (Debian)
    Connect with a web browser to:
	http://localhost:631
    And configure printer (HP example shown) to:
	HP LaserJet 2600n, Foomatic + foo2zjs (en)
    Then edit "Manage Printers->Configure Printer" to suit you,
    such as "Page Size" or "Color Mode".

Create printers (Solaris 11+)
    # printmgr

Create printers (command line using CUPS)
    # lpadmin -p "NAME" -v "URI" -E -P file.ppd.gz
    i.e.
	# lpadmin -p hp1020 -v "usb://HP/LaserJet%201020" -E \
	    -P /usr/share/cups/model/HP-LaserJet_1020.ppd.gz
    Set the default:
	# lpadmin -d "NAME"

Create at least one queue for monochrome, and another queue
for color printing.  Create the queues, then edit them and
set the "device options" as desired.

For a networked Minolta/QMS 2300 DL, I used a "Queue Type"
of "Unix Printer (LPD)", and set the "Server" to the IP address
of the printer, and the "Queue" to "lp".

For a networked HP Color Laserjet 2600n, I used a "Queue Type"
of "Networked JetDirect", and set the "Printer" to the IP address
of the printer, and the "Port" to "9100".

GHOSTSCRIPT BUGS
----------------
    * ghostscript 8.64 is broken w.r.t. color.  Don't use!

    * ghostscript 9.00 is broken w.r.t. fonts in landscape mode.

    * ghostscript 9.+ is broken w.r.t. color. Don't use

    * Well Tempered Screening (WTS) works with ghostscript 8.54 thru 8.70+.
      So if you want BEST COLORS, you'll have to install gs 8.54 or better
      if you don't have it.

	OPTIONAL: 
	    # yum install cups-devel
		-OR-
	    $ sudo apt-get install cups-dev

	$ gs --version
	8.15.2
	
	$ wget "http://ghostscript.com/releases/ghostscript-8.71.tar.gz"
	$ tar zxf ghostscript-8.71.tar.gz
	$ cd ghostscript-8.71
	$ ./autogen.sh
	$ make
	$ su				OR $ sudo cp bin/gs /usr/bin/gs.foo
	# cp bin/gs /usr/bin/gs.foo

	(Optional)
	# make install			OR $ sudo make install

	$ gs.foo --version
	8.71

      If that doesn't compile (e.g. Ubuntu 11.10+), try this:
	$ cd ghostscript-8.71
	$ ./configure  --without-jbig2dec
	$ make CFLAGS+="-DHAVE_SYS_TIME_H=1"

    * Halftoning Bug:
        "The problems with WTS are primarily that it seems to fall down
	on the halftone generation for some angles when the lpi is high for
	the current resolution." - Ray Johnston <ray.johnston@artifex.com>

	So choose Standard, Accurate Screens, or reduce the resolution to
	600x600.

    * Ghostscript before 8.55 has a problem with ICM files and 64-bit gcc.
      It causes a segfault with km2430_2.icm. So don't select that one.

FEDORA NOTES 
------------
    Install tix, foomatic\*, and system-config-printer FIRST:
	# yum install tix foomatic\* system-config-printer

    If you are using a USB printer AND Fedora 12+, do this:

	# grep udev-configure-printer /var/log/messages
	/var/log/messages:Jan 23 07:32:54 dual udev-configure-printer: \
    		invalid or missing IEEE 1284 Device ID

	# rpm -e --nodeps system-config-printer-udev

	# shutdown -r now

	Power off then on the printer.

    Ref:
	http://bugzilla.redhat.com/show_bug.cgi?id=558162

UBUNTU NOTES
------------
    Install build-essential, tix, foomatic-filters, groff, dc FIRST:
	$ sudo apt-get install build-essential tix foomatic-filters groff dc

	$ wget -O foo2zjs.tar.gz http://foo2zjs.rkkda.com/foo2zjs.tar.gz
	$ tar zxf foo2zjs.tar.gz
	$ cd foo2zjs
	$ sudo make uninstall
	$ make
	$ ./getweb 1020
	    OR other printer
	$ sudo make install install-hotplug cups

	For 7.10 and later users:
	    $ sudo system-config-printer

	For 5.10/6.06/6.10/7.04 users:
	    $ sudo gnome-cups-manager
	    [configure ColorMode = Color if a color printer]
	    $ sudo make cups

	    Ubuntu has a bug in gnome-cups-manager with Color, so you must
	    restart cups.  No other distro has this bug.

    If that doesn't work, then fire up:
	$ firefox http://localhost:631

	And click on:
	    Printers -> Set Printer Options -> Color Mode -> Color
	Then click on:
	    Set Printer Options

DEBIAN NOTES
------------
    Install build-essential, tix, foomatic-filters, groff, cupsys, dc FIRST:
	$ su
	# apt-get install build-essential tix foomatic-filters groff dc
	# apt-get install cups		# For all others
	    OR
	# apt-get install cupsys	# For lenny and earlier

	$ wget -O foo2zjs.tar.gz http://foo2zjs.rkkda.com/foo2zjs.tar.gz
        $ tar zxf foo2zjs.tar.gz
        $ cd foo2zjs
        $ make
        $ ./getweb 1020
            OR other printer
        $ su
        # make install install-hotplug cups

	$ firefox http://localhost:631

OPENSUSE 1x.x NOTES
-------------------
    Do this:

	# zypper install make gcc

	# zypper service-add \
	    http://download.opensuse.org/repositories/Printing/openSUSE_11.3/ \
	    Printing
	# zypper up -r Printing -t package
    
    Then install using the above instructions.

ACER ASPIRE ONE NOTES
---------------------

    Ref: http://the.taoofmac.com/media/Acer/Aspire\ One/AA1notes.htm

    It is a version of Fedora.

	Get a shell by typing Alt+F2 then Return.

	$ su
	# yum install make gcc
	<ctrl-d>

	$ wget -O foo2zjs.tar.gz http://foo2zjs.rkkda.com/foo2zjs.tar.gz
        $ tar zxf foo2zjs.tar.gz
        $ cd foo2zjs
        $ make
        $ ./getweb 1020
            OR other printer, e.g. 2600n
	$ su
        # make install install-hotplug cups

    
ASUS EEE PC NOTES
-----------------

    It is a version of Xandros.  First:

	Get a shell by typing ctrl-alt-T
	$ sudo su -
	# vi or kwrite /etc/apt/sources.list
	    add the following line:
		deb ftp://ftp.us.debian.org/debian stable main contrib non-free
	# apt-get -f install
	# apt-get install wget
	# apt-get install build-essential
	<ctrl-d>

	$ wget -O foo2zjs.tar.gz http://foo2zjs.rkkda.com/foo2zjs.tar.gz
        $ tar zxf foo2zjs.tar.gz
        $ cd foo2zjs
        $ make
        $ ./getweb 1020
            OR other printer, e.g. 2600n
        $ sudo make install install-hotplug cups

    Then use the "Add Printer" GUI.

MAC OS X NOTES
---------------
    Please read the detailed installation instructions by Clint Morgan
    and Rick Richardson in the file INSTALL.osx.

FREEBSD NOTES
-------------
    You need the following packages before you start the "make":
	# pkg_add -r wget
	# pkg_add -r gmake
	# pkg_add -r ghostscript-gnu
	# pkg_add -r cups
	# pkg_add -r foomatic-filters
	# pkg_add -r unzip

    Use "gmake" instead of "make".  E.G. gmake; ./getweb XXX; gmake install

    USB NOTES FOR FREEBSD 8.0 AND GREATER
    -------------------------------------
	$ gmake
	$ ./getweb 1020
            OR other printer, e.g. 2600n
	# gmake install install-hotplug
	# ./freebsd-install

	Use:
	    usb:/dev/ulpt0	Device with reset #0
	    usb:/dev/unlpt0	Device without reset #0
	    usb:/dev/ulpt1	Device with reset #1
	    usb:/dev/unlpt1	Device without reset #1
	for the URI.

	More information:
	    http://menhennitt.com.au/wordpress/2009/09/27/printing-to-an-hp-laserjet-1020-from-freebsd-8-using-cups-and-foo2zjs
	    http://farid.hajji.name/blog/2010/02/02/printing-woes-on-freebsd-8-with-cups/

    USB NOTES FOR FREEBSD 7.x AND LESSER
    ------------------------------------
	- Build the kernel without the ulpt driver. 
	    e.g.
	    # vi /usr/src/sys/i386/conf/GENERIC
		comment out 'device ulpt'
	    # cd /usr/src/
	    # make buildkernel KERNCONF=GENERIC
	    # make installkernel KERNCONF=GENERIC
	    reboot

	- Do one of these lines each time the HP printer is powered up:
	    # cat /usr/share/foo2zjs/firmware/sihp1018.dl > /dev/ugen0.1
	    # cat /usr/share/foo2zjs/firmware/sihp1020.dl > /dev/ugen0.1
	    # cat /usr/share/foo2xqx/firmware/sihpP1005.dl > /dev/ugen0.1
	    # cat /usr/share/foo2xqx/firmware/sihpP1006.dl > /dev/ugen0.1
	    # cat /usr/share/foo2xqx/firmware/sihpP1505.dl > /dev/ugen0.1

	More information:
	    http://www.webmiscreants.com/index.php?page=howto_P1006

OPENBSD NOTES
-------------
    You need the following packages before you start the "make":
	# pkg_add wget
	# pkg_add gmake
	# pkg_add -i ghostscript
	# pkg_add cups
	# pkg_add unzip

    Use "gmake" instead of "make".  E.G. gmake; ./getweb XXX; gmake install

    USB NOTES FOR OPENBSD
	- Build the kernel without the ulpt driver. 
	    e.g.
	    # vi /usr/src/sys/i386/conf/GENERIC
		comment out 'device ulpt'
	    # cd /usr/src/
	    # make buildkernel KERNCONF=GENERIC
	    # make installkernel KERNCONF=GENERIC
	    reboot

	- Do one of these lines each time the printer is powered up:
	    # cat /usr/share/foo2zjs/firmware/sihp1018.dl > /dev/ugen0.1
	    # cat /usr/share/foo2zjs/firmware/sihp1020.dl > /dev/ugen0.1
	    # cat /usr/share/foo2xqx/firmware/sihpP1005.dl > /dev/ugen0.1
	    # cat /usr/share/foo2xqx/firmware/sihpP1006.dl > /dev/ugen0.1
	    # cat /usr/share/foo2xqx/firmware/sihpP1505.dl > /dev/ugen0.1

OPENSOLARIS, SOLARIS EXPRESS DEVELOPER EDITION 9/07, Solaris 11+ NOTES
----------------------------------------------------------------------
    Use "bash" for your shell.  Only network printers are supported.

    $ export PATH=$PATH:/sbin:/usr/sbin:/usr/sfw/bin:/opt/sfw/bin
    
    Do this:

	[ Load CD Solaris_Software_Companion]
	$ cd /media/S10_807_SOFTWARE_COMPANION/Solaris_Software_Companion/Solaris_i386/Packages
	$ su root -c "/usr/bin/bash"
	# pkgadd -d `pwd` SFWgroff
	# pkgadd -d `pwd` SFWgawk

    OR
	Browse to:
	    http://pkg.opensolaris.org/release/en/index.shtml
	and Search or Browse Packages and download:

	    SUNWscp
	    SUNWgawk
	    SUNWgroff

    Then:

    $ wget -O foo2zjs.tar.gz http://foo2zjs.rkkda.com/foo2zjs.tar.gz
    $ tar zxf foo2zjs.tar.gz
    $ cd foo2zjs

    $ gmake
    $ ./getweb 2530
	OR other printer

    $ su root -c "/usr/bin/bash"
    # gmake install
    # printmgr

    To see a screen to the GUI:
	http://foo2lava.rkkda.com/solaris/

    NOTE: you cannot see the printer options (Paper Source, Paper Type,
    Paper Media, Color Mode, ICM, etc.).  There is NO GUI to do it!!!
    Sorry.

MINOLTA-QMS 2200/2300 DL NOTES
------------------------------
    Use the network interface if you can.  These printers understand Unix
    LPD printer server protocol.  So when setting up the printer queue,
    you can select "UNIX Printer (lpd queue)", set the lpd queue name to
    "lp" (arbitrary), and set the "Server" to the IP address of the
    printer.

    These printers also understand several other printer server protocols,
    such as JetDirect and IPP, but I have not tried them.  In any case,
    I'm not aware of any advantages of using them over LPD.

    The USB interface on this printer will work if your printer is at
    firmware revision 2.55 or later.  Mine was not, but I was able to
    get this firmware from the Konica Minolta Europe web site.  The USA
    site doesn't have it.  Upgrading the firmware on your printer can
    be dangerous and might turn your printer into a paperweight, so I do
    not recommend it unless you need USB and are a computer expert.  To
    get the v2.55 firmware upgrade, try:
	./getweb 2300dl_fw

CUPS USB NOTES
--------------
    If you are using the USB port, then the URI should be:
	file:/dev/usb/lp0	OR	usb:/dev/usb/lp0
	file:/dev/usb/lp1	OR	usb:/dev/usb/lp1
    OR
	usb://Samsung/CLP-310%20Series
	usb://Samsung/CLP-310%20Series
	usb://HP/Color%20LaserJet%20CP1215
	usb://HP/Color%20LaserJet%202600n
	usb://HP/LaserJet%201000
	usb://HP/LaserJet%201005
	usb://HP/LaserJet%201018
	usb://HP/LaserJet%201020
	usb://HP/LaserJet%20P1005
	usb://HP/LaserJet%20P1006
	usb://HP/LaserJet%20P1007
	usb://HP/LaserJet%20P1008
	usb://HP/LaserJet%20P1505
	usb://HP/LaserJet%20Professional%20P1102w

    Don't use hp://<whatever> because that is for hplip (a closed source,
    proprietary driver).

    Do a "make cups" as root if you haven't done it before.

HP LASERJET 1000/1005/1018/1020, P1005/P1006/P1007/P1008/P1505 NOTES
--------------------------------------------------------------------
    These printers need their firmware downloaded to them every time they
    are powered up.

	On Linux with USB connected printer:
	    If you are running Linux and the printer is connected via USB, you
	    can arrange for the firmware to be automatically downloaded to the
	    printer by performing one more installation step:

	    # make install-hotplug

	    Power off then on the printer. Light should flash orange for
	    ~5 seconds as the firmware is getting downloaded.

	On another OS or with a parallel port connected printer:

	    You must send a firmware file to the printer each time you power it
	    up.  If you downloaded the extra files for the HP above, a typical
	    command line to load the firmware would be ONE of these:

	    # cat /usr/share/foo2zjs/firmware/sihp1000.dl > /dev/usb/lp0
	    # cat /usr/share/foo2zjs/firmware/sihp1005.dl > /dev/usb/lp0
	    # cat /usr/share/foo2zjs/firmware/sihp1018.dl > /dev/usb/lp0
	    # cat /usr/share/foo2zjs/firmware/sihp1020.dl > /dev/usb/lp0
	    # cat /usr/share/foo2xqx/firmware/sihpP1005.dl > /dev/usb/lp0
	    # cat /usr/share/foo2xqx/firmware/sihpP1006.dl > /dev/usb/lp0
	    # cat /usr/share/foo2xqx/firmware/sihpP1505.dl > /dev/usb/lp0

	    Light should flash orange for ~5 seconds as the firmware is
	    getting downloaded.

	On Mac OS X:

	    You must send a firmware file to the printer each time you power it
	    up.  If you downloaded the extra files for the HP above, a typical
	    command line to load the firmware would be:

		$ lp -oraw /usr/share/foo2zjs/firmware/sihp1018.dl
		$ lp -oraw /usr/share/foo2zjs/firmware/sihp1020.dl
		$ lp -oraw /usr/share/foo2xqx/firmware/sihpP1005.dl
		$ lp -oraw /usr/share/foo2xqx/firmware/sihpP1006.dl
		$ lp -oraw /usr/share/foo2xqx/firmware/sihpP1505.dl

	    -OR-

		Add a line to /etc/rc.local and reboot:

		    killall osx-hplj-hotplug; \
			osx-hplj-hotplug >/tmp/osx-hplj-hotplug 2>&1 &

	    -OR-

		Issue a "make install-hotplug" command:
	    
		$ sudo make install-hotplug

	    Light should flash orange for ~5 seconds as the firmware is
	    getting downloaded.

    Firmware Not Downloaded:
	# usb_printerid /dev/usb/lp0
	GET_DEVICE_ID string:
	MFG:Hewlett-Packard;MDL:HP LaserJet 1020;CMD:ACL;CLS: PRINTER;\
		    DES:HP LaserJet 1020;

    Firmware Downloaded:
	# usb_printerid /dev/usb/lp0
	GET_DEVICE_ID string:
	MFG:Hewlett-Packard;MDL:HP LaserJet 1020;CMD:ACL;CLS: PRINTER;\
		    DES:HP LaserJet 1020;FWVER:20050309;

    NOTE: The original HP files are named '*.img'.  Sometimes HP supplies
    these files ready-to-download to the printer, sometimes they are raw
    ARM executables and need to have a special header added to them before
    they can be downloaded.  The "make install" step will use the supplied
    "arm2hpdl" program to automatically detect which kind of file they are
    and convert them (if needed) to the downloadable '*.dl' format.

    These printers do not have a "button" when you run out of paper.
    But, there is a GNOME gui in:

	Applications -> System Tools -> HPLJ 10xx Replaced Paper

    It requires tcl, tk, and tix.  Fedora 5 and later:
	# yum install tcl tk tix

    or, you can simulate this by reloading the paper and doing:

	$ usb_printerid /dev/usb/lp0

    or, you can open the print cartridge door and then close it.

HP SMART INSTALL NOTES
----------------------
    The printers HP LaserJet Pro P1102, HP LaserJet Pro CP1025, and simliar
    models have a virtual CD-ROM (a fake USB CD drive) in USB mode.  You can
    disable this three ways:

    Method 1:
	NOTE: this is a non-open-source method!
	- Connect the printer to a Windows PC and turn it on.
	  The fake CD-ROM appears on Windows.
	- Insert the original Driver CD that ships with the printer
	- Run SIUtility.exe or SIUtility64.exe from the UTIL folder and
	  COMPLETELY DISABLE THIS "HP SMART INSTALL" FEATURE. 

    Method 2:
	- Install usb_modeswitch and usb_modeswitch-data from your distro's
	  repository. I.E.:
	    # yum install usb_modeswitch usb_modeswitch-data
	  OR
	    $ sudo apt-get install usb-modeswitch-data
	  OR
	    Surf to: http://www.draisberghof.de/usb_modeswitch/
	- Power cycle the printer.

    Method 3:
	NOTE: this is a non-open-source method!
	- Execute:
	    $ wget http://hplipopensource.com/hplip-web/smartinstall/\
		SmartInstallDisable-Tool.run
	    $ sh SmartInstallDisable-Tool.run

PSUTILS AND 2/4-UP CAPABILITY
-----------------------------
    If you would like to use the 2-up/4-up capability, then you need to
    get and install Angus Duggan's excellent psutils package.  You can
    find the source code for psutils here:

	http://knackered.knackered.org/angus/psutils/index.html

    Or an RPM here:

	http://rpmfind.net/linux/rpm2html/search.php?query=psutils

CUSTOM PAGE SIZE
----------------

    Append "PageSize=Custom.MMMxNNNin" to the lpr command.  E.G.

    $ lpr -P hp2600 -o media=letter -o PageSize=Custom.4x6in ~/testpage.ps
    $ lpr -P hp2600 -o media=letter -o PageSize=Custom.10x15cm ~/testpage.ps
    $ lpr -P hp1020 -o media=letter -o PageSize=Custom.4x6in ~/testpage.ps

    Or, use a GUI that allows the custom size parameters, e.g.
    "evince" - PostScript and PDF File Viewer.

LANDSCAPE ORIENTATION
---------------------
    This driver just prints Postscript and doesn't know what the
    orientation is (*).  Other higher level programs format your
    data into Postscript, e.g CUPS. 

    The CUPS -o landscape option will rotate the page 90 degrees to print
    in landscape orientation:

    $ lp -o landscape filename
    $ lpr -o landscape filename

    (*) except for N-up printing, because psnup (from psutils) requires it!

SET DEFAULT MEDIA WITH CUPS
---------------------------
    $ sudo
    # lpoptions -o media=A4
	-OR-
    # lpoptions -o media=Letter

MANUAL DUPLEX
-------------

    See:
	https://sourceforge.net/projects/g-manual-duplex/

	Install:
	    $ make
	    $ su
	    # make install      -OR-    $ sudo make install
	    [logout]
	    [login]

	Then:
	    Using the Gnome 2 or Gnome-3 Classic (fallback) GUI:
	    1a)     System Tools -> Gnome Manual Duplex
		    - OR -
	    1b)     Add to Panel -> Gnome Manual Duplex applet -> Add
	    2)      Print -> GnomeManualDuplex (Virtual Printer) -> Print

	    Using the Gnome 3 Shell GUI:
	    1)      $ gnome-session-properties
		    Startup Programs -> GnomeManualDuplex -> Enable
		    [logout][login]
	    2)      Print -> GnomeManualDuplex (Virtual Printer) -> Print

	    Works with *.ps and *.pdf files.
	    Works with Gnome-2 or Gnome-3.

	- Print odd pages
	- Wait for confimation message
	- Insert in the same orientation into the printer
	- Print reverse even pages

	Howto (video):
	    http://www.youtube.com/watch?v=c4Ghomz6RQI

    -OR-
	$ psmandup [options] file.ps
	
	Ref:
	    Fedora: # yum install a2ps
	    Ubuntu: $ sudo apt-get install a2ps

    -OR- (Gnome)
	Print -> Page Setup -> Only print -> Odd Sheets

	then:

	Print -> Page Setup -> Only print -> Even Sheets

    -OR- (Gnome)
	Print -> Job -> Odd Pages

	then:

	Print -> Job -> Even Pages 

    -OR- (KDE)
	Okular -> Print -> Copies -> Page Set -> Odd Pages

	then:

	Okular -> Print -> Copies -> Page Set -> Even Pages

    Ref:
	http://bugzilla.gnome.org/show_bug.cgi?id=520598

UPDATE
------
    Here are handy lines you can click on to get the latest version:

	http://foo2zjs.rkkda.com/
	wget http://foo2zjs.rkkda.com/foo2zjs.tar.gz

    My advice: update early and often!!!!

UNINSTALLING
------------
    This will uninstall everything from your system.

    $ su
    # make uninstall

BUG REPORTS
-----------
    PLEASE use the forums at:
	http://foo2zjs.rkkda.com/forum/index.php

    I do not read or reply to HTML email or messages sent under an alias.
    I failed out of french class, so don't even think about sending
    me email in anything but English.

    Rick Richardson

DEVELOPER AND DEBUGGING TIPS
----------------------------
    If you want to work on this program, I recommend creating a "raw"
    printer queue directed at the printer, with no protocol conversions.
    OR, simple copy the file to /dev/usb/lp0 (USB) or nc (netcat) the
    file (network).

    Then, you can use the "foo2zjs-wrapper" program to convert Postscript
    test programs to ZjS format, and inspect them with "zjsdecode" before
    deciding whether to print them or not.  For example:

	foo2zjs-wrapper testpage.ps > testpage.zm
	foo2zjs-wrapper -c testpage.ps > testpage.zc

	zjsdecode < testpage.zm
	zjsdecode < testpage.zc

	lpr -Praw testpage.zm
	    OR
	cp testpage.zm /dev/usb/lp0
	    OR
	nc 192.168.1.NNN 9100 < testpage.zm

    Same thing for the other drivers, e.g. ...

	foo2hiperc-wrapper testpage.ps > testpage.hc
	hipercdecode < testpage.hc
	nc 192.168.1.NNN 9100 < testpage.hc

    If the printer is an HP LaserJet 10xx or P1xxx and needs to have the
    firmware downloaded, this will tell you (P1006):
	Before:
	    usb_printerid /dev/usb/lp0
	    MFG:Hewlett-Packard;MDL:HP LaserJet P1006;CMD:ACL;CLS:PRINTER;\
		DES:HP LaserJet P1006;

	After:
	    usb_printerid /dev/usb/lp0
	    MFG:Hewlett-Packard;MDL:HP LaserJet P1006;CMD:ACL;CLS:PRINTER;\
		DES:HP LaserJet P1006;FWVER:20080415;

CUSTOM ICC/ICM COLOR PRINTER PROFILE (BUY)
------------------------------------------

    I need:
	Dell 1355 or Xerox 6015		default resolution
	Samsung CLP-315			default resolution
	Samsung CLP-325			default resolution
	Samsung CLP-360 or 365		default resolution
	Samsung CLP-600			default resolution
	Samsung CLP-610			default resolution
	Samsung CLP-620			default resolution
	HP Color LaserJet 1500		default resolution
	HP Color LaserJet CP1215	default resolution, 1-bit and 2-bit
	HP Color LaserJet 2600n		2-bit, default resolution

    NOTE:
    This works only if you have ghostscript 8.x. If you have gs 9.x, then
    read "GHOSTSCRIPT BUGS" and prepare /usr/bin/gs.foo from gs 8.x.

    0)	Pick a vendor, e.g.
	    google: "Custom Printer Profiles"

	    MadManChan's Custom Printer Profiles
	    http://people.csail.mit.edu/ericchan/photos/profiles.html
	    Cost: 20 dollars

	    PC35 PhotoLab Custom Printer Profiling Services
	    http://printerprofiles.homestead.com/
	    Cost: 30 dollars

	    Cathy's Profiles
	    http://www.cathysprofiles.com/
	    Cost: 35 dollars

	    "Custom ICC ICM colour printer profile RGB or CMYK"
	    Seller: personalised101
	    http://stores.ebay.ie/The-Graphics-Depot 
	    Cost: 10 pounds

	    "We Create a Custom ICC Profile for Your Printer-"
	    Seller: fotojimbo
	    http://search.ebay.com/_W0QQsassZfotojimbo
	    Cost: 10 dollars

	    "Custom Color ICC Profile Printer Epson HP Canon 3800"
	    Seller: Booksmart Studio
	    http://stores.shop.ebay.com/Booksmart-Studio
	    Cost: 25 dollars

    1)	Convert the vendor sheet(s) from *.tif to page*.ps (OPTIONAL)

	    $ gimp

		OR

	    Preferred, using ImageMagick's "convert"
	    $ convert Color\ Patch\ RGB\ \(Page\ 1\).tif page1.ps
	    $ convert Color\ Patch\ RGB\ \(Page\ 2\).tif page2.ps

		OR

	    From *.jpg to *.ps
	    $ convert a300DPI_i1-RGB-1.5.jpg -rotate 90 -density 300x300 \
		-quality 100 page1.ps

    2)	Print the Postscript vendor sheet(s) with NO color correction:

	    $ foo2hp2600-wrapper -c -C10 -Gnone.icm page1.ps > test1.prn

	    $ nc 192.168.1.xxxxxxx 9100 < test1.prn
		OR
	    $ cp test1.prn /dev/usb/lp0

	    repeat for page2.ps (if necessary).

    3)	Send them to the vendor by POSTAL MAIL

    4)	Get back *.icc/*.icm profile by EMAIL or WEB

    5)	Put it in /usr/share/foo2hp/icm/testing.icm

    6)	Print a test picture:

	    $ foo2hp2600-wrapper -c -C10 -Gtesting.icm \
		picture.ps > picture.prn

	    $ nc 192.168.1.xxxxxxx 9100 < picture.prn
		OR
	    $ cp picture.prn /dev/usb/lp0

    7)	If it is OK, send "testing.icm" to rick.richardson@comcast.net
	for inclusion in foo2zjs.

    Other printers: use foo2qpdl-wrapper and /usr/share/foo2qpdl/icm/
    Other printers: use foo2lava-wrapper and /usr/share/foo2lava/icm/

CUSTOM ICC/ICM COLOR PRINTER PROFILE (ARGYLL)
---------------------------------------------
    NOTE:
    This works only if you have ghostscript 8.x. If you have gs 9.x, then
    read "GHOSTSCRIPT BUGS" and prepare /usr/bin/gs.foo from gs 8.x.

    Reference:
	firefox http://www.xritephoto.com/html/colormunkisplash.htm
	firefox http://www.argyllcms.com/
	man printer-profile

    DON'T DO THIS ON A 32-BIT (i386) PROCESSOR!
	Ghostscript (8.63) has problems.  Weird color profile data.

    ONLY DO THIS ON A 64-BIT (x86_64)PROCESSOR.
	But, you can use the color profile on i386 and x86_64.

    YOU HAVE BEEN WARNED!!!

    Execute:
	$ man printer-profile
	$ printer-profile  manuf model [rgb|cmyk] [patches] [ink-limit]

    If it is OK, send "testing.icm" to rick.richardson@comcast.net
	for inclusion in foo2zjs.
