---
title: Qwen
description: Qwen model configuration (Text / Image Understanding / Image Generation / Speech-to-Text / Text-to-Speech / Embedding)
---

Qwen (Alibaba DashScope / Bailian) is one of the most fully-featured providers. Text, image understanding, image generation, speech-to-text, text-to-speech, and embedding can all be enabled with a single `dashscope_api_key`.

<Tip>
  All capabilities below can be configured in one place via the "Model Management" page in the Web Console, with no need to manually edit the configuration file.
</Tip>

## Text Chat

```json
{
  "model": "qwen3.7-plus",
  "dashscope_api_key": "YOUR_API_KEY"
}
```

| Parameter | Description |
| --- | --- |
| `model` | Can be `qwen3.7-plus`, `qwen3.7-max`, `qwen3.6-plus`, `qwen3.5-plus`, `qwen3-max`, `qwen-max`, `qwen-plus`, `qwen-turbo`, `qwq-plus`, etc. |
| `dashscope_api_key` | Create one in the [Bailian Console](https://bailian.console.aliyun.com/?tab=model#/api-key); see the [official docs](https://bailian.console.aliyun.com/?tab=api#/api) |

## Image Understanding

Once `dashscope_api_key` is configured, the Agent's Vision tool automatically calls Qwen's vision models to recognize images. Models like `qwen3.7-plus` / `qwen3.6-plus` / `qwen3.5-plus` / `qwen3-max` are already multimodal; if the main model is text-only (e.g. `qwen-turbo`), it automatically falls back to `qwen-vl-max`.

To manually specify a Vision model:

```json
{
  "tools": {
    "vision": {
      "model": "qwen3.7-plus"
    }
  }
}
```

Supported models: `qwen3.7-plus`, `qwen3.6-plus`, `qwen3.5-plus`, `qwen3-max`.

## Image Generation

```json
{
  "skills": {
    "image-generation": {
      "model": "qwen-image-2.0"
    }
  }
}
```

Available models: `qwen-image-2.0`, `qwen-image-2.0-pro`.

## Speech-to-Text (ASR)

```json
{
  "voice_to_text": "dashscope",
  "voice_to_text_model": "qwen3-asr-flash"
}
```

| Parameter | Description |
| --- | --- |
| `voice_to_text` | Set to `dashscope` to enable Qwen ASR |
| `voice_to_text_model` | Optional, defaults to `qwen3-asr-flash` |

Credentials are automatically reused from `dashscope_api_key`. A single audio segment should be smaller than 10MB and no longer than 300 seconds.

## Text-to-Speech (TTS)

```json
{
  "text_to_voice": "dashscope",
  "text_to_voice_model": "qwen3-tts-flash",
  "tts_voice_id": "Cherry"
}
```

| Parameter | Description |
| --- | --- |
| `text_to_voice_model` | Optional, defaults to `qwen3-tts-flash`; covers Mandarin, dialects, and major foreign languages |
| `tts_voice_id` | Voice ID; see the common list below |

Common voice examples:

| Voice ID | Description |
| --- | --- |
| `Cherry` | Qianyue · Sunny Female Voice |
| `Serena` | Suyao · Gentle Female Voice |
| `Ethan` | Chenxu · Sunny Male Voice |
| `Chelsie` | Qianxue · Anime Girl |
| `Dylan` | Beijing Dialect · Xiaodong |
| `Rocky` | Cantonese · Aqiang |
| `Sunny` | Sichuan Dialect · Qing'er |

The full voice list (Mandarin / regional dialects / bilingual, etc.) can be selected visually in the Web Console under "Model Management → Text-to-Speech".

## Embedding

```json
{
  "embedding_provider": "dashscope",
  "embedding_model": "text-embedding-v4"
}
```

The default model is `text-embedding-v4`. After changing the embedding, run `/memory rebuild-index` to rebuild the index.
