# Instructions for ML Brass

ML Brass can be downloaded here: https://www.waverunneraudio.com/shop/pisces-rising-ml-brass/

Before you continue, download the .SFZ mapping from the "ML Brass SFZ File" folder.

## How to use the sfz mapping

1. In order to use Kontakt libraries with .NCW files, you need to use Kontakt to extract them.
<br><img src="images/Capture.PNG" width="60%"><br>
Navigate to this menu, and click the button highlighted above.

2. Press "OK"
<br><img src="images/Capture2.PNG" width="60%">

3. Click the folder button and navigate to the ML Brass folder. It's the folder with the .NKI file in it.
<br><img src="images/Capture3.PNG" width="60%">
<img src="images/Capture4.PNG" width="60%"><br>
I would recommend setting the destination folder to a different folder called "ML Brass SFZ" or something similar to that.

4. Now that you have the files, you need to put the ML Brass.sfz file in the folder that the "ML Brass Samples" folder is in.
<br><img src="images/Capture5.PNG" width="60%">

5. Now you should delete the files with endings like "-[1]", like the ones highlighted below.
<br><img src="images/Capture6.PNG" width="60%">

6. Lastly, you need to rename this file, change the end from "_03", to "_02".
<br><img src="images/Capture7.PNG" width="60%">

That's it, enjoy!
