| OrbbecSDK 1.10.18 OrbbecSDK: Software-Development-Kit for Orbbec 3D Cameras

Loading...
Searching...
No Matches
Public Attributes | List of all members
OBDataChunk Struct Reference

Structure for transmitting data blocks. More...

`#include <ObTypes.h>`

## Public Attributes
uint8_t * | data
| Pointer to current block data.
uint32_t | size
| Length of current block data.
uint32_t | offset
| Offset of current data block relative to complete data.
uint32_t | fullDataSize
| Size of full data.

## Detailed Description

Structure for transmitting data blocks.

Definition at line 315 of file ObTypes.h.

## Member Data Documentation

## ◆ data

uint8_t* OBDataChunk::data

Pointer to current block data.

Definition at line 316 of file ObTypes.h.

## ◆ size

uint32_t OBDataChunk::size

Length of current block data.

Definition at line 317 of file ObTypes.h.

## ◆ offset

uint32_t OBDataChunk::offset

Offset of current data block relative to complete data.

Definition at line 318 of file ObTypes.h.

## ◆ fullDataSize

uint32_t OBDataChunk::fullDataSize

Size of full data.

Definition at line 319 of file ObTypes.h.

The documentation for this struct was generated from the following file:

- E:/Projects/Jenkins/workspace/OrbbecSDK/libobsensor/include/libobsensor/h/ObTypes.h