| OrbbecSDK 1.10.18 OrbbecSDK: Software-Development-Kit for Orbbec 3D Cameras

Loading...
Searching...
No Matches
Public Attributes | List of all members
HDR_CONFIG Struct Reference

HDR Configuration. More...

`#include <ObTypes.h>`

## Public Attributes
uint8_t | enable
| Enable/disable HDR, after enabling HDR, the exposure_1 and gain_1 will be used as the first exposure and gain, and the exposure_2 and gain_2 will be used as the second exposure and gain. The output image will be alternately exposed and gain between the first and second exposure and gain.
uint8_t | sequence_name
| Sequence name.
uint32_t | exposure_1
| Exposure time 1.
uint32_t | gain_1
| Gain 1.
uint32_t | exposure_2
| Exposure time 2.
uint32_t | gain_2
| Gain 2.

## Detailed Description

HDR Configuration.

Definition at line 1449 of file ObTypes.h.

## Member Data Documentation

## ◆ enable

uint8_t HDR_CONFIG::enable

Enable/disable HDR, after enabling HDR, the exposure_1 and gain_1 will be used as the first exposure and gain, and the exposure_2 and gain_2 will be used as the second exposure and gain. The output image will be alternately exposed and gain between the first and second exposure and gain.

Attention
  After enabling HDR, the auto exposure will be disabled.

Definition at line 1458 of file ObTypes.h.

## ◆ sequence_name

uint8_t HDR_CONFIG::sequence_name

Sequence name.

Definition at line 1459 of file ObTypes.h.

## ◆ exposure_1

uint32_t HDR_CONFIG::exposure_1

Exposure time 1.

Definition at line 1460 of file ObTypes.h.

## ◆ gain_1

uint32_t HDR_CONFIG::gain_1

Gain 1.

Definition at line 1461 of file ObTypes.h.

## ◆ exposure_2

uint32_t HDR_CONFIG::exposure_2

Exposure time 2.

Definition at line 1462 of file ObTypes.h.

## ◆ gain_2

uint32_t HDR_CONFIG::gain_2

Gain 2.

Definition at line 1463 of file ObTypes.h.

The documentation for this struct was generated from the following file:

- E:/Projects/Jenkins/workspace/OrbbecSDK/libobsensor/include/libobsensor/h/ObTypes.h