| dp14 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDp_SbMsgLinkAddressReplyDeviceInfo Struct Reference
Overview

This typedef describes a DisplayPort branch device. More...

## Data Fields
u8 | Guid [XDP_GUID_NBYTES]
| The global unique identifier (GUID) of the branch device. More...
u8 | NumPorts
| The number of ports associated with this branch device. More...
XDp_SbMsgLinkAddressReplyPortDetail | PortDetails [XDP_MAX_NPORTS]
              An
array describing all ports attached to this branch device. More...

## Detailed Description

This typedef describes a DisplayPort branch device.

This structure is used when the driver is operating in multi-stream transport (MST) mode.

## Field Documentation

u8 XDp_SbMsgLinkAddressReplyDeviceInfo::Guid[XDP_GUID_NBYTES]

The global unique identifier (GUID) of the branch device.

u8 XDp_SbMsgLinkAddressReplyDeviceInfo::NumPorts

The number of ports associated with this branch device.

XDp_SbMsgLinkAddressReplyPortDetail XDp_SbMsgLinkAddressReplyDeviceInfo::PortDetails[XDP_MAX_NPORTS]

              An

array describing all ports attached to this branch device.