| dfeprach Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfePrach_CCSequence Struct Reference
Overview

Defines a CCID sequence. More...

## Data Fields
u32 | Length
| [1-16] Sequence length More...
s32 | CCID [XDFEPRACH_SEQ_LENGTH_MAX]
       [0-15].Array of CCID's
arranged in the order the CCIDs are required to be processed in the PRACH. More...

## Detailed Description

Defines a CCID sequence.

## Field Documentation

s32 XDfePrach_CCSequence::CCID[XDFEPRACH_SEQ_LENGTH_MAX]

       [0-15].Array of CCID's

arranged in the order the CCIDs are required to be processed in the PRACH.

May contain duplicate entries depending on the rate channel rates.

Referenced by XDfePrach_GetCarrierCfgMB(), and XDfePrach_GetEmptyCCCfg().

u32 XDfePrach_CCSequence::Length

[1-16] Sequence length

Referenced by XDfePrach_2CC3RCDynamicTestExample(), XDfePrach_2CC3RCReconfigureTestExample(), XDfePrach_2CC3RCTestExample(), XDfePrach_GetCarrierCfgMB(), XDfePrach_GetEmptyCCCfg(), and XDfePrach_Initialize().