| v_hdmirx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XV_HdmiRx_Config Struct Reference

This typedef contains configuration information for the HDMI RX core. More...

## Data Fields
u16 | DeviceId
| DeviceId is the unique ID of the HDMI RX core. More...
UINTPTR | BaseAddress
| BaseAddress is the physical base address of the core's registers. More...

## Detailed Description

This typedef contains configuration information for the HDMI RX core.

Each HDMI RX device should have a configuration structure associated.

## Field Documentation

UINTPTR XV_HdmiRx_Config::BaseAddress

BaseAddress is the physical base address of the core's registers.

Referenced by XV_HdmiRx_CfgInitialize(), XV_HdmiRx_ClearLinkStatus(), XV_HdmiRx_DdcGetEdidWords(), XV_HdmiRx_DdcGetHdcpReadMessageBufferWords(), XV_HdmiRx_DdcGetHdcpWriteMessageBufferWords(), XV_HdmiRx_DdcIsHdcpReadMessageBufferEmpty(), XV_HdmiRx_DdcIsHdcpWriteMessageBufferEmpty(), XV_HdmiRx_DdcLoadEdid(), XV_HdmiRx_GetAcrCts(), XV_HdmiRx_GetAcrN(), XV_HdmiRx_GetAviColorSpace(), XV_HdmiRx_GetAviVic(), XV_HdmiRx_GetGcpColorDepth(), XV_HdmiRx_GetLinkStatus(), XV_HdmiRx_GetTmdsClockRatio(), XV_HdmiRx_GetVideoProperties(), XV_HdmiRx_GetVideoTiming(), XV_HdmiRx_IntrHandler(), XV_HdmiRx_IsLinkStatusErrMax(), XV_HdmiRx_SelfTest(), XV_HdmiRx_SetColorFormat(), XV_HdmiRx_SetHpd(), XV_HdmiRx_SetPixelRate(), and XV_HdmiRx_WriteScdcRegister().

u16 XV_HdmiRx_Config::DeviceId

DeviceId is the unique ID of the HDMI RX core.