| v_sdirx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XV_SdiRx_Config Struct Reference

This typedef contains configuration information for the SDI RX core. More...

## Data Fields
u16 | DeviceId
| DeviceId is the unique ID of the SDI RX core. More...
UINTPTR | BaseAddress
| BaseAddress is the physical base address of the core's registers. More...

## Detailed Description

This typedef contains configuration information for the SDI RX core.

Each SDI RX device should have a configuration structure associated.

## Field Documentation

UINTPTR XV_SdiRx_Config::BaseAddress

BaseAddress is the physical base address of the core's registers.

Referenced by XV_SdiRx_Axi4sBridgeDisable(), XV_SdiRx_Axi4sBridgeEnable(), XV_SdiRx_CfgInitialize(), XV_SdiRx_ClearYCbCr444_RGB_10bit(), XV_SdiRx_DebugInfo(), XV_SdiRx_FramerDisable(), XV_SdiRx_FramerEnable(), XV_SdiRx_GetIntrEnable(), XV_SdiRx_GetIntrStatus(), XV_SdiRx_GetPayloadId(), XV_SdiRx_GetSdiMode(), XV_SdiRx_InterruptClear(), XV_SdiRx_IntrDisable(), XV_SdiRx_IntrEnable(), XV_SdiRx_ReportDetectedError(), XV_SdiRx_SelfTest(), XV_SdiRx_SetYCbCr444_RGB_10bit(), XV_SdiRx_Start(), XV_SdiRx_Stop(), XV_SdiRx_VidBridgeDisable(), XV_SdiRx_VidBridgeEnable(), XV_SdiRx_WaitforPayLoad(), and XV_SdiRxSelfTestExample().

u16 XV_SdiRx_Config::DeviceId

DeviceId is the unique ID of the SDI RX core.