| v_hdmiphy1 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XHdmiphy1_Hdmi21Cfg Struct Reference
Overview

This typedef contains the HDMI 2.1 FRL configurations. More...

## Data Fields
u8 | IsEnabled
| Is HDMI operation is enabled? More...
u64 | LineRate
| Linerate in bps. More...
u8 | NChannels
| No of Channels. More...

## Detailed Description

This typedef contains the HDMI 2.1 FRL configurations.

## Field Documentation

u8 XHdmiphy1_Hdmi21Cfg::IsEnabled

Is HDMI operation is enabled?

Referenced by XHdmiphy1_ClkDetGetRefClkFreqHz(), XHdmiphy1_Hdmi20Config(), XHdmiphy1_Hdmi21Config(), XHdmiphy1_HdmiCpllParam(), XHdmiphy1_HdmiGtTxResetDoneLockHandler(), XHdmiphy1_HdmiQpllParam(), XHdmiphy1_HdmiRxClkDetFreqChangeHandler(), XHdmiphy1_HdmiRxTimerTimeoutHandler(), XHdmiphy1_HdmiTxClkDetFreqChangeHandler(), XHdmiphy1_HdmiTxTimerTimeoutHandler(), and XHdmiphy1_SetHdmiTxParam().

u64 XHdmiphy1_Hdmi21Cfg::LineRate

Linerate in bps.

Referenced by XHdmiphy1_Hdmi20Config(), XHdmiphy1_Hdmi21Config(), XHdmiphy1_HdmiCpllParam(), and XHdmiphy1_HdmiQpllParam().

u8 XHdmiphy1_Hdmi21Cfg::NChannels

No of Channels.

Referenced by XHdmiphy1_Hdmi20Config(), XHdmiphy1_Hdmi21Config(), XHdmiphy1_HdmiGtTxResetDoneLockHandler(), and XHdmiphy1_HdmiTxClkDetFreqChangeHandler().