| v_hdmitxss1 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Data Structures | Enumerations | Functions
onsemi_nb7nq621m.h File Reference

## Data Structures
struct | Onsemi_RegisterField
| This typedef contains translations of FRL_Rate to Lanes and Line Rates. More...

## Enumerations
enum | Onsemi_DeviceType
| FRL Character Rate Enumeration. More...

## Functions
int | ONSEMI_NB7NQ621M_Init (void *IicPtr, u8 I2CSlaveAddress, u8 Revision, u8 IsTx)
| This function initializes the ONSEMI NB7NQ621M with default values for use with the Video FMC. More...
int | ONSEMI_NB7NQ621M_CheckDeviceID (void *IicPtr, u8 I2CSlaveAddress)
| This function checks the ONSEMI NB7NQ621M device ID. More...
u8 | ONSEMI_NB7NQ621M_CheckDeviceVersion (void *IicPtr, u8 I2CSlaveAddress)
| This function checks the ONSEMI NB7NQ621M Device Revision Number. More...
int | ONSEMI_NB7NQ621M_LineRateReconfig (void *IicPtr, u8 I2CSlaveAddress, u8 Revision, u8 IsFRL, u64 LineRate, u8 IsTx)
| This function reconfigures the ONSEMI NB7NQ621M cable redriver. More...
void | ONSEMI_NB7NQ621M_RegisterDump (void *IicPtr, u8 I2CSlaveAddress)
| This function displays a registerdump of the ONSEMI NB7NQ621M device. More...
void | ONSEMI_NB7NQ621M_RegisterLibraryDump (void)
| This function prints out all the contents from OnsemiRegisterFields array. More...