| dp14 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDp_TxVscExtPacket Struct Reference
Overview

This typedef contains the VSC extended packet information. More...

## Data Fields
u32 | BitsPerColor
| Number of bits per color color component. More...
u8 | ComponentFormat
| The component format currently in use by the video stream. More...
u8 | DynamicRange
| The dynamic range currently in use by the video stream. More...
u8 | YCbCrColorimetry
| The YCbCr colorimetry currently in use by the video stream. More...
u32 | Header
| VSC packet header. More...

## Detailed Description

This typedef contains the VSC extended packet information.

## Field Documentation

u32 XDp_TxVscExtPacket::BitsPerColor

Number of bits per color color component.

u8 XDp_TxVscExtPacket::ComponentFormat

The component format currently in use by the video stream.

u8 XDp_TxVscExtPacket::DynamicRange

The dynamic range currently in use by the video stream.

u32 XDp_TxVscExtPacket::Header

VSC packet header.

u8 XDp_TxVscExtPacket::YCbCrColorimetry

The YCbCr colorimetry currently in use by the video stream.