| dfemix Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeMix_Phase Struct Reference
Overview

Defined phase for single CC's NCO. More...

## Data Fields
u32 | PhaseAcc
| [0-2^32-1] Phase accumulator value More...
u32 | DualModCount
| [0-2^32-1] Dual modulus count value (T-S) More...
u32 | DualModSel
| [0,1] Dual modulus select value More...
u32 | TriggerUpdateFlag
                    Update the associated accumulator from
the PHASE registers: More...

## Detailed Description

Defined phase for single CC's NCO.

## Field Documentation

u32 XDfeMix_Phase::DualModCount

[0-2^32-1] Dual modulus count value (T-S)

u32 XDfeMix_Phase::DualModSel

[0,1] Dual modulus select value

u32 XDfeMix_Phase::PhaseAcc

[0-2^32-1] Phase accumulator value

u32 XDfeMix_Phase::TriggerUpdateFlag

                    Update the associated accumulator from

the PHASE registers:

- 0 = NO_UPDATE: Do not update
- 1 = IMMEDIATE_UPDATE: Apply an immediate update
- 2 = TRIGGER_UPDATE: Apply an update on the next CC_UPDATE trigger