| usbpsu Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XUsbPsu_Event_Gevt Struct Reference
USBPSU APIs

struct XUsbPsu_event_gevt - Other Core Events More...

## Data Fields
u32 | Is_GlobalEvt: 1
| non-endpoint event (not used) More...
u32 | Device_Event: 7
| it's (0x03) Carkit or (0x04) I2C event More...
u32 | Phy_Port_Number: 4
| Phy_Port_Number:4. More...
u32 | Reserved31_12: 20
| reserved31_12 More...

## Detailed Description

struct XUsbPsu_event_gevt - Other Core Events

Parameters

  one_bit,: | indicates this is a non-endpoint event (not used)
  device_event,: | indicates it's (0x03) Carkit or (0x04) I2C event.
  phy_port_number,: | self-explanatory
  reserved31_12,: | Reserved, not used.

## Field Documentation

u32 XUsbPsu_Event_Gevt::Device_Event

it's (0x03) Carkit or (0x04) I2C event

u32 XUsbPsu_Event_Gevt::Is_GlobalEvt

non-endpoint event (not used)

u32 XUsbPsu_Event_Gevt::Phy_Port_Number

Phy_Port_Number:4.

u32 XUsbPsu_Event_Gevt::Reserved31_12

reserved31_12