| dfeofdm Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeOfdm_ModelParameters Struct Reference
Overview

OFDM model parameters structure. More...

## Data Fields
u32 | NumAntenna
| [1-8] Number of antennas More...
u32 | AntennaInterleave
| [1-8] Antenna interleave More...
u32 | PhaseCompensation
| [0,1] Phase compensation More...

## Detailed Description

OFDM model parameters structure.

Data defined in Device tree or xparameters.h for BM.

## Field Documentation

u32 XDfeOfdm_ModelParameters::AntennaInterleave

[1-8] Antenna interleave

Referenced by XDfeOfdm_AddCCExample(), XDfeOfdm_Configure(), and XDfeOfdm_MultiAddCCExample().

u32 XDfeOfdm_ModelParameters::NumAntenna

[1-8] Number of antennas

Referenced by XDfeOfdm_AddCCExample(), XDfeOfdm_Configure(), and XDfeOfdm_MultiAddCCExample().

u32 XDfeOfdm_ModelParameters::PhaseCompensation

[0,1] Phase compensation

- 0: Phase compensation disabled
- 1: Phase compensation enabled

Referenced by XDfeOfdm_Configure().