| v_hdmirxss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
Overview

## Functions
int | XV_HdmiRxSs_SubcoreInitHdmiRx (XV_HdmiRxSs *HdmiRxSsPtr)
| This function initializes the included sub-core to it's static configuration. More...
XV_HdmiRxSs_Config * | XV_HdmiRxSs_LookupConfig (u32 DeviceId)
| This function looks for the device configuration based on the unique device ID. More...

## Function Documentation

XV_HdmiRxSs_Config* XV_HdmiRxSs_LookupConfig | ( | u32 | DeviceId | ) |

This function looks for the device configuration based on the unique device ID.

The table XV_HdmiRxSs_ConfigTable[] contains the configuration information for each instance of the device in the system.

Parameters

  DeviceId | is the unique device ID of the device being looked up

Returns
  A pointer to the configuration table entry corresponding to the given device ID, or NULL if no match is found

int XV_HdmiRxSs_SubcoreInitHdmiRx | ( | XV_HdmiRxSs * | HdmiRxSsPtr | ) |

This function initializes the included sub-core to it's static configuration.

Parameters

  HdmiRxSsPtr | is a pointer to the Subsystem instance to be worked on.

Returns
  XST_SUCCESS/XST_FAILURE

References XV_HdmiRxSs_SubCore::AbsAddr, XV_HdmiRxSs_Config::BaseAddress, XV_HdmiRxSs::Config, XV_HdmiRxSs_SubCore::DeviceId, XV_HdmiRxSs::EdidLength, XV_HdmiRxSs::EdidPtr, XV_HdmiRxSs_Config::HdmiRx, XV_HdmiRxSs::HdmiRxPtr, XV_HDMIRXSS_LOG_EVT_HDMIRX_INIT, and XV_HdmiRxSs_LogWrite().

Referenced by XV_HdmiRxSs_CfgInitialize().